[Contents] [Prev] [Next] [Index] [Report an Error]

# graceful-restart notify-time

#### Syntax

[ no ] graceful-restart notify-time notifyTime

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the estimated time for the OSPFv2 router to send purged grace LSAs over all interfaces. The no version returns the notify duration timer to its default value, 15 seconds.

#### Options

- notifyTime—Number of seconds during which the router can send purged grace LSAs over all interfaces; in the range 1–1800

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]