> - Download PDFs
> - udp-port
> - Related Topics
> - Configuring RADIUS-Based Mirroring

> # udp-port

> #### Syntax

> udp-port port

> no udp-port

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> From RADIUS Configuration mode, specifies the UDP port on the router where the RADIUS authentication, accounting, or dynamic-request servers reside. The router uses this port to communicate with the RADIUS servers. The no version restores the default value.

> From RADIUS Relay Configuration mode, specifies the UDP port on the router where the RADIUS relay authentication or accounting server resides. The router uses this port to communicate with the RADIUS relay servers. The no version restores the default value.

> #### Options

> - port—Port number in the range 1–65535
>   - 1812—Default for RADIUS and RADIUS relay authentication servers
>   - 1813—Default for RADIUS and RADIUS relay accounting servers
>   - 1700—Default for RADIUS dynamic-request servers

> #### Mode

> RADIUS Configuration, RADIUS Relay Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.