[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 nd ra-interval

#### Syntax

ipv6 nd ra-interval seconds

no ipv6 nd ra-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
Profile Configuration mode added in JUNOSe Release 9.0.0.

#### Description

Specifies the interval between IPv6 router advertisement retransmissions on an interface. The no version restores the default interval, 200 seconds.

#### Options

- seconds—Number of seconds between IPv6 advertisement retransmissions; in the range 3–1800

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]