[Contents] [Prev] [Next] [Index] [Report an Error]

# path ds3 t1 timeslots

#### Syntax

path pathChannel ds3 ds3Channel t1 t1Channel/subchannel timeslots range
[ speed { 56 | 64 } ]

no path pathChannel ds3 ds3Channel t1 t1Channel/subchannel

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Assigns a range of DS0 timeslots to a subchannel as a single data stream for a T1 channel on a DS3 signal. This command applies to a T1 channel on a DS3 over channelized SONET interface. You can optionally specify a line speed that applies to all DS0 timeslots assigned to a subchannel. The no version deletes the fractional T1 circuit.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the DS3 channel
- t1Channel—Number, in the range 1–28, that identifies the T1 channel
- subchannel—Fractional T1 interface, in the range 1–24
- range—Timeslots assigned to the T1 channel in the range 1–24; a dash represents a range of timeslots, and a comma separates timeslots. For example, 1-10, 15-18 assigns timeslots 1–10 and 15–18.
- speed—Specifies the data rate for the T1 channel, either 56 Kbps or 64 Kbps; default value is 64 Kbps

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]