[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuring DHCP Relay

The Dynamic Host Configuration Protocol (DHCP) provides a mechanism through which computers using Transmission Control Protocol/IP (TCP/IP) can obtain protocol configuration parameters automatically from a DHCP server on the network.

The following sections describe how to configure your E-series router to provide DHCP support:

- Configuring DHCP Relay and BOOTP Relay
- Configuring DHCP Relay Proxy

[Contents] [Prev] [Next] [Index] [Report an Error]