[Contents] [Prev] [Next] [Index] [Report an Error]

# hello-interval

#### Syntax

hello-interval helloInterval

no hello-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the interval between hello packets that the router sends on the OSPF remote-neighbor interface. The no version restores the default value.

#### Options

- helloInterval—Number in the range 1–65535 seconds; default value is 10 seconds

#### Mode

Remote Neighbor Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]