[Contents] [Prev] [Next] [Index] [Report an Error]

# ntp broadcast-delay

#### Syntax

ntp broadcast-delay delayTime

no ntp broadcast-delay

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the estimated round-trip delay between the broadcast NTP server and the router. The no version restores the round-trip delay to the default value, 3000 microseconds.

#### Options

- delayTime—Value in the range 0–999999 microseconds

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]