[Contents] [Prev] [Next] [Index] [Report an Error]

# Disabling Per-Port Queuing on ATM Interfaces

You can remove per-port queuing on ATM interfaces and restore the default integrated mode setting.

When per-port queuing is disabled, both the VC and port backpressure are enabled. The SAR scheduler performs significant buffering, and the HRR scheduler does minimal scheduling. The atm-vc node command must appear in the QoS profile attached to the ATM port.

To disable per-port queuing:

1. Specify the ATM interface for which you want to disable per-port queuing.
   `
   host1(config)#interface atm 2/0
   `
2. Disable per-port queuing on that interface.
   `
   host1(config-if)#no qos-mode-port
   `

#### Related Topics

- Configuring Default Integrated Mode for ATM Interface
- interface atm command
- qos-mode-port command

[Contents] [Prev] [Next] [Index] [Report an Error]