[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls atm vci range

#### Syntax

mpls atm vci range minVCI maxVCI

no mpls atm vci range

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the range for virtual circuit identifiers that can be used in MPLS labels for an MPLS major interface on an ATM AAL5 interface using the interface label space. Creates the MPLS major interface if it does not yet exist. An error message is generated if you issue the command for any other layer 2 interface, as they do not support the interface label space. The no version deletes the range.

#### Options

- minVCI—Lowest virtual circuit identifier acceptable for a label, a value from 33–65535
- maxVCI—Highest virtual circuit identifier acceptable for a label, a value from 33–65535

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]