[Contents] [Prev] [Next] [Index] [Report an Error]

# mask destination

#### Syntax

mask destination destinationMinimumSize

no mask destination

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Sets the minimum mask size for the destination address for the prefix and destination prefix aggregation caches. The no version restores the default mask size.

#### Options

- destinationMinimumSize—Mask number in the range 1—32; default is 0

#### Mode

Flow Cache Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]