[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

A B C D E F G H I J L M N P Q R S T U V

A

> access lists, IP 1
>   specifying multicast groups 1
> access lists, IPv6 1
>   specifying multicast groups 1
> advertising DVMRP routes 1
> assert messages 1
> assigning multicast groups 1
> auto-RP router 1
>   PIM sparse mode 1
>   PIM sparse-dense mode 1

B

> baseline commands 1
>   baseline ip dvmrp 1
>   baseline ip igmp 1
>   baseline ip igmp-proxy interface 1
>   baseline ipv6 mld 1
>   baseline ipv6 mld-proxy interface 1
> BFD (Bidirectional Forwarding Detection) 1
>   RIP, configuring for 1
> BGP multicasting 1

C

> Class D IPv4 addresses 1
> clear ip commands 1
>   clear ip dvmrp route 1
>   clear ip mroute 1
>   clear ip pim auto-rp 1
>   clear ip pim interface count 1
>   clear ip pim remote-neighbor count 1
> clear ipv6 commands 1
>   clear ipv6 mroute 1
>   clear ipv6 pim remote-neighbor count 1
> conventions 1
>   notice icons 1
>   text and syntax 1
> customer support 1
>   contacting JTAC 1

D

> data MDT, creating 1
> data path failure 1
>   detecting RIP 1
> debug commands 1
>   debug ip pim 1
>   debug ipv6 pim 1
> default MDT, creating 1
> detecting RIP data path failure 1
> disable command 1
> disable-dynamic-redistribute command 1
>   DVMRP 1
> disabling dynamic route redistribution 1
>   DVMRP 1
> Distance Vector Multicast Routing Protocol. 1, See DVMRP
> documentation set 1
>   comments on 1
> downstream interface 1
> DRs (designated routers) 1
>   PIM routing 1
> DVMRP (Distance Vector Multicast Routing Protocol) 1
>   advertising routes 1
>   configuring 1
>     limits 1
>     summary addresses 1
>   default router, configuring 1
>   deleting routes 1
>   enabling 1
>     on a virtual router 1
>     on an interface 1
>   exchanging unicast routes 1
>   filtering reports 1
>   metric 1
>   monitoring 1
>   neighbors 1
>   overview 1
>   pruning 1
>   summary addresses 1
>   tunnels 1
>   using with IGMP 1
>   using with PIM 1
> dynamic route redistribution, disabling 1
>   in DVMRP 1

E

> encapsulation commands 1
>   encapsulation vlan 1
> exchanging DVMRP unicast routes 1

F

> filtering 1
>   DVMRP reports 1

G

> group membership 1
>   queries 1
>   reports 1

H

> hardware multicast packet replication 1
>   monitoring 1
>   OIF mapping 1
>   overview 1
> hello interval 1
>   PIM 1
> hold time 1
>   PIM sparse mode 1
> hop count 1

I

> IGMP (Internet Group Management Protocol) 1
>   configuring 1
>   disabling 1
>   enabling 1
>   limiting groups on interfaces 1
>   monitoring 1
>   performing host functions 1
>   querier 1
>   removing 1
>   specifying version 1
> igmp commands 1
>   igmp disable 1
>   igmp promiscuous 1
> IGMP proxy 1
>   configuring 1
>   enabling 1
>   monitoring 1
>   version 1
> IGMP reports, accepting 1
> IGP (interior gateway protocol) 1
> importing routes. 1, See redistributing routes
> Internet Group Management Protocol. 1, See IGMP
> investigating IP multicast routes 1
> IP addresses 1
>   class D 1
>   for multicasting 1
> ip commands 1
>   ip block-multicast-sources 1
>   ip multicast-routing 1
>   ip multicast-routing disable-rpf-check 1
>   ip multicast-routing permanent-mroute 1
>   ip route-type 1
>   ip rpf-route 1
>   ip unnumbered 1
>   mroute port limit 1
> ip dvmrp commands 1
>   ip dvmrp 1
>   ip dvmrp accept-filter 1
>   ip dvmrp announce-list 1
>   ip dvmrp auto-summary 1
>   ip dvmrp disable 1
>   ip dvmrp metric-offset 1
>   ip dvmrp route-limit 1
>   ip dvmrp routehog-notification 1
>   ip dvmrp summary-address 1
>   ip dvmrp unicast-routing 1
>   See also
> ip igmp commands 1
>   ip igmp 1
>   ip igmp access-group 1
>   ip igmp access-source-group 1
>   ip igmp group limit 1
>   ip igmp immediate-leave 1
>   ip igmp last-member query-interval 1
>   ip igmp promiscuous 1
>   ip igmp querier 1
>   ip igmp querier-timeout 1
>   ip igmp query-interval 1
>   ip igmp query-max-response-time 1
>   ip igmp robustness 1
>   ip igmp ssm-map enable 1
>   ip igmp ssm-map static 1
>   ip igmp static-exclude 1
>   ip igmp static-group 1
>   ip igmp static-include 1
>   ip igmp version 1
>   ip igmp-proxy 1
>   ip igmp-proxy unsolicited-report-interval 1
>   ip igmp-proxy V1-router-present-time 1
>   See also
> ip multicast commands 1
>   ip multicast admission-bandwidth-limit 1
>   ip multicast ioa-packet-replication 1
>   ip multicast-routing bandwidth-map 1
> IP multicast groups 1
>   assigning to an interface 1
>   identifying 1
>   leaving 1
>   maintaining membership of 1
>   reporting 1
>   specifying 1
> IP multicast interfaces, monitoring 1
> IP multicast routes 1
> IP multicasting 1
>   benefits of 1
>   deleting routes 1
>   enabling 1
>   M-BONE 1
>   monitoring 1
> ip pim commands 1
>   ip pim 1
>   ip pim bsr-candidate 1
>   ip pim data-mdt 1
>   ip pim group-address-pool 1
>   ip pim join-filter 1
>   ip pim query-interval 1
>   ip pim rp-address 1
>   ip pim rp-candidate 1
>   ip pim send-rp-announce 1
>   ip pim send-rp-discovery scope 1
>   ip pim sparse-mode graceful-restart-duration 1
>   ip pim spt-threshold 1
>   See also
> ip rip commands 1
>   ip rip bfd-liveness-detection 1
> IP tunnels 1
>   monitoring 1
> ipv6 commands 1
>   ip route-type 1
>   ipv6 block-multicast-sources 1
>   ipv6 mld robustness 1
>   ipv6 multicast-routing 1
>   ipv6 multicast-routing disable-rpf-check 1
>   ipv6 multicast-routing permanent-route 1
>   ipv6 rpf-route 1
>   See also
> ipv6 mld commands 1
>   ipv6 mld 1
>   ipv6 mld access-group 1
>   ipv6 mld access-source-group 1
>   ipv6 mld apply-oif-map 1
>   ipv6 mld explicit-tracking 1
>   ipv6 mld group limit 1
>   ipv6 mld immediate-leave 1
>   ipv6 mld last-member query-interval 1
>   ipv6 mld oif-map 1
>   ipv6 mld querier-timeout 1
>   ipv6 mld query-interval 1
>   ipv6 mld query-max-response-time 1
>   ipv6 mld ssm-map enable 1
>   ipv6 mld ssm-map static 1
>   ipv6 mld static-exclude 1
>   ipv6 mld static-group 1
>   ipv6 mld static-include 1
>   ipv6 mld version 1
>   ipv6 mld-proxy 1
>   ipv6 mld-proxy unsolicited-report-interval 1
>   ipv6 mld-proxy version 1
>   See also
> IPv6 multicast 1
>   benefits of 1
>   deleting routes 1
>   enabling 1
>   monitoring 1
> ipv6 multicast commands 1
>   ipv6 multicast admission-bandwidth-limit 1
>   ipv6 multicast ioa-packet-replication 1
>   ipv6 multicast-routing bandwidth-map 1
> IPv6 multicast groups 1
>   assigning to an interface 1
>   identifying 1
>   leaving 1
>   maintaining membership of 1
>   reporting 1
>   specifying 1
> ipv6 pim commands 1
>   ipv6 pim 1
>   ipv6 pim bsr-candidate 1
>   ipv6 pim join-filter 1
>   ipv6 pim query-interval 1
>   ipv6 pim rp-address 1
>   ipv6 pim rp-candidate 1
>   ipv6 pim spt-threshold 1
>   See also

J

> join messages 1

L

> leave group membership messages 1
> leaving an IP multicast group 1
> leaving an IPv6 multicast group 1
> limiting IGMP groups on interfaces 1
> limiting MLD groups on interfaces 1
> liveness detection 1
>   RIP and BFD 1

M

> M-BONE (multicast backbone of the Internet) 1
> manuals 1
>   comments on 1
> MDT (Multicast Distribution Tree) 1
>   creating with default MDT 1
> mdt commands 1
>   mdt-data-delay 1
>   mdt-data-holddown 1
>   mdt-data-timeout 1
>   mdt-interval 1
> metric 1
>   DVMRP 1
> MLD (Multicast Listener Discovery) 1
>   configuring 1
>   disabling 1
>   enabling 1
>   limiting groups on interfaces 1
>   monitoring 1
>   performing host functions 1
>   removing 1
>   specifying version 1
> mld disable command 1
> MLD proxy 1
>   configuring 1
>   enabling 1
>   monitoring 1
>   version 1
> mrinfo requests, support for 1
> mtrace command 1
> multicast 1
>   IP. 1, See IP multicasting
>   IPv6. 1, See IPv6 multicast
> Multicast Distribution Tree. 1, See MDT
> multicast group port limit command 1
> Multicast Listener Discovery. 1, See MLD
> multicast VPNs 1
>   creating with data MDTs 1
>   creating with the default MDT 1
>   overview 1

N

> neighbors, DVMRP 1
> notice icons 1

P

> PIM (Protocol Independent Multicast) 1
>   displaying events 1
>   enabling 1
>     on a virtual router 1
>     on an interface 1
>   monitoring 1
>   removing 1
>   resetting counters and mappings 1
>   using with DVMRP 1
>   using with IGMP 1
>   using with MLD 1
>   See also
> PIM dense mode 1
>   See also
> pim disable command 1
> PIM SM. 1, See PIM sparse mode
> PIM sparse mode 1
>   configuring auto-RP router 1
>   joining groups 1
>   pruning 1
>   remote neighbors, configuring 1
>   setting a threshold 1
>   timers 1
> PIM sparse-dense mode 1
>   configuring auto-RP router 1
>   overview 1
> PIM SSM (PIM source-specific multicast) 1
>   enabling 1
>   requirements for IGMPv3 1
>   requirements for MLDv2 1
> Protocol Independent Multicast. 1, See PIM
> prune messages 1

Q

> query-interval command 1

R

> reachability commands 1
>   IP multicast 1
> redistribute command 1
>   DVMRP 1
> redistributing routes, DVMRP 1
> redistribution routes 1
>   disabling dynamic (DVMRP) 1
> remote neighbors 1
>   PIM sparse mode 1
>     configuring 1
> remote-neighbor command 1
> removing PIM 1
> rendezvous point router. 1, See RP routers
> reporting IP multicast groups 1
> reporting IPv6 multicast groups 1
> resetting PIM counters and mappings 1
> reverse-path forwarding. 1, See RPF
> RIP (Routing Information Protocol) 1
>   BFD liveness detection and 1
>   detecting path failures 1
>   purging learned routes 1
> route-map command 1
> router commands 1
>   router dvmrp 1
>   router igmp 1
>   router mld 1
>   router pim 1
> routes 1
>   using for other protocols 1
> routing policy commands 1
>   set admission-bandwidth 1
>   set qos-bandwidth 1
> RP (rendezvous point) routers 1
>   assigning automatically 1
>   configuring 1
>     automatic 1
>     static 1
> RPF (reverse-path forwarding) 1
> RPF routes, monitoring 1

S

> set threshold command 1
> setting 1
>   baseline 1
>     DVMRP 1
>     IGMP 1
>     IGMP Proxy 1
>     MLD 1
>     MLD Proxy 1
>   DVMRP hop-count 1
>   PIM SPT threshold 1
>     IP 1
>     IPv6 1
> shared trees 1
> shortest path trees. 1, See SRTs
> show ip commands 1
>   show ip mroute 1
>   show ip mroute count 1
>   show ip mroute summary 1
>   show ip rpf-route 1
> show ip dvmrp commands 1
>   show ip dvmrp 1
>   show ip dvmrp interface 1
>   show ip dvmrp mroute 1
>   show ip dvmrp neighbor 1
>   show ip dvmrp route 1
>   show ip dvmrp routeNextHop 1
> show ip igmp commands 1
>   show ip igmp 1
>   show ip igmp groups 1
>   show ip igmp interface 1
>   show ip igmp interface brief 1
>   show ip igmp membership 1
>   show ip igmp-proxy 1
>   show ip igmp-proxy groups 1
>   show ip igmp-proxy interface 1
> show ip multicast commands 1
>   show ip multicast protocols 1
>   show ip multicast protocols brief 1
>   show ip multicast routing 1
> show ip pim commands 1
>   show ip pim 1
>   show ip pim auto-rp 1
>   show ip pim bsr 1
>   show ip pim data-mdt 1
>   show ip pim dense-mode sg-state 1
>   show ip pim interface 1
>   show ip pim neighbor 1
>   show ip pim rp 1
>   show ip pim rp-hash 1
>   show ip pim sparse-mode sg-state 1
>   show ip pim sparse-mode unicast-route 1
>   show ip pim spt-threshold 1
> show ipv6 commands 1
>   show ipv6 mroute 1
>   show ipv6 mroute count 1
>   show ipv6 mroute summary 1
>   show ipv6 rpf-route 1
> show ipv6 mld commands 1
>   show ipv6 mld 1
>   show ipv6 mld groups 1
>   show ipv6 mld interface 1
>   show ipv6 mld interface brief 1
>   show ipv6 mld membership 1
>   show ipv6 mld-proxy 1
>   show ipv6 mld-proxy groups 1
>   show ipv6 mld-proxy interface 1
> show ipv6 mld ssm-mapping command 1
> show ipv6 multicast commands 1
>   show ipv6 multicast protocols 1
>   show ipv6 multicast protocols brief 1
>   show ipv6 multicast routing 1
> show ipv6 pim commands 1
>   show ipv6 pim 1
>   show ipv6 pim bsr 1
>   show ipv6 pim interface 1
>   show ipv6 pim neighbor 1
>   show ipv6 pim remote-neighbor 1
>   show ipv6 pim rp 1
>   show ipv6 pim rp-hash 1
>   show ipv6 pim sparse-mode sg-state 1
>   show ipv6 pim sparse-mode unicast-route 1
>   show ipv6 pim spt-threshold 1
> show multicast group limit command 1
> source-rooted trees. 1, See SRTs
> Source-Specific Multicast for IP—draft-ietf-ssm-arch-06.txt (March 2005 expiration) 1
> specifying IP multicast groups 1
> specifying IPv6 multicast groups 1
> SPTs (shortest path trees). 1, See SRTs
> SRTs (source-rooted trees) 1
> static routes 1
>   configuring 1
> summary addresses 1
>   DVMRP routing 1
> support, technical 1, See technical support

T

> technical support 1
>   contacting JTAC 1
> text and syntax conventions 1
> timers 1
>   PIM sparse mode 1
> trace packets 1
> tunnel group-address-pool command 1
> tunnel mdt command 1

U

> undebug commands 1
>   undebug ip pim 1
>   undebug ipv6 pim 1
> unicast routes, DVMRP 1
> update-source command 1
> upstream interface 1

V

> vlan commands 1
>   encapsulation vlan 1

[Contents] [Prev] [Next] [Index] [Report an Error]