[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls ldp egress-label

#### Syntax

mpls ldp egress-label { explicit-null | non-null }

no mpls ldp egress-label

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Configures LDP to advertise the explicit null label (label 0) or a non-null label for the LSR that is the egress router for the prefix. This command takes effect immediately. The no version restores the default, where the egress router advertises the implicit null label (label 3), which causes the router's upstream neighbor to perform a penultimate hop pop.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]