[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring BFD

You configure BFD on routing protocols that use BFD for fast failure detection. BFD does not require any stand-alone configuration; it works in conjunction with the application that it is supporting. Applications on which you configure BFD pass configuration information to BFD when they need fast failure detection.

BFD works with a wide variety of routing protocols. The JUNOSe software currently supports only a few of these protocols. All BFD supported clients provide the ability to configure session parameters for each interface. Refer to the following table for added configuration information:

Configuration Topic | See
--- | ---
EBGP | Chapter Configuring BGP Routing in JUNOSe BGP and MPLS Configuration Guide
IPv4 static routes | Chapter Configuring IP in JUNOSe IP, IPv6, and IGP Configuration Guide
IS-IS | Chapter Configuring IS-IS in JUNOSe IP, IPv6, and IGP Configuration Guide
OSPF | Chapter Configuring OSPF in JUNOSe IP, IPv6, and IGP Configuration Guide
OSPFv3 | Chapter Configuring OSPF in JUNOSe IP, IPv6, and IGP Configuration Guide
PIM | Chapter Configuring PIM for IPv4 Multicast in JUNOSe IP, IPv6, and IGP Configuration Guide and chapter Configuring PIM for IPv6 Multicast in JUNOSe Multicast Routing Configuration Guide
RIP | Chapter Configuring RIP in JUNOSe IP, IPv6, and IGP Configuration Guide
RSVP-TE | Chapter Configuring MPLS in JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]