[Contents] [Prev] [Next] [Index] [Report an Error]

# Spoof Checking MPLS Packets

The MPLS forwarding table enables MPLS to determine whether an MPLS packet received from an upstream neighbor contains an MPLS label that was advertised to that neighbor. If not, the packet is dropped. Each entry in the forwarding table has a spoof check field that specifies the type of checking that must be performed for the associated in label. The signaling protocol (BGP, LDP, or RSVP) that populates the entry in the MPLS forwarding table sets the spoof check field.

MPLS supports the following types of spoof checking:

- Router spoof checking—MPLS packets are accepted only if they arrive on an MPLS major interface that is in the same virtual router as the MPLS forwarding table.
- Interface spoof checking—MPLS packets are accepted only if they arrive on the particular MPLS major interface identified in the spoof check field.

You can use the show mpls forwarding command to view the spoof check field for an MPLS forwarding table entry.

#### Related Topics

- MPLS Forwarding and Next-Hop Tables

[Contents] [Prev] [Next] [Index] [Report an Error]