[Contents] [Prev] [Next] [Index] [Report an Error]

# path ds3 t1 framing

#### Syntax

path pathChannel ds3 ds3Channel t1 t1Channel framing framingType

no path pathChannel ds3 ds3Channel t1 t1Channel framing

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the framing format for a T1 channel on a DS3 signal. This command applies to a T1 channel on a DS3 over channelized SONET interface. The no version restores the default value.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the DS3 channel
- t1Channel—One or more individual T1 channels, ranges of T1 channels, or combination of individual channels and ranges, in the range 1–28 (no spaces); for example, 3,7-15,19-13,27
- framingType—One of the following types:
  - esf—Default; specifies extended superframe
  - sf—Specifies superframe

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]