[Contents] [Prev] [Next] [Index] [Report an Error]

# Before You Configure VPWS

The JUNOSe software implementation of VPWS uses features of BGP, MPLS, BGP/MPLS VPNs, and layer 2 services over MPLS. We recommend you have a thorough understanding of these protocols before you configure and use VPWS in your network.

#### Related Topics

For more information about configuring BGP, MPLS, BGP/MPLS VPNs, and layer 2 services over MPLS, see the following chapters in this guide:

- Configuring BGP Routing
- Configuring MPLS
- Configuring BGP-MPLS Applications
- Layer 2 Services over MPLS Overview
- Configuring Layer 2 Services over MPLS
- Monitoring Layer 2 Services over MPLS
- For more information about configuring the layer 2 interfaces that support L2VPNs, see Configuration Tasks for Ethernet in the JUNOSe Physical Layer Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]