[Contents] [Prev] [Next] [Index] [Report an Error]

# isis network point-to-point

#### Syntax

[ no ] isis network point-to-point

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the IS-IS circuit type as point-to-point. Issuing this command tears down existing adjacencies, originates or flushes LSPs, and establishes new adjacencies. The no version restores the default, treating the circuit as a broadcast circuit.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]