[Contents] [Prev] [Next] [Index] [Report an Error]

# delta-sampling

#### Syntax

delta-sampling [ discontinuity-id mibId
| discontinuity-id-type { timeStamp | timeTicks } ]

no delta-sampling [ discontinuity-id ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies delta sampling for the trigger you are configuring. The no version returns the trigger to the default sampling method—absolute-value sampling.

#### Options

- discontinuity-id—Specifies a discontinuity MIB ID for the sample. The discontinuity MIB ID monitors the sample for any discontinuity errors during the sample frequency. If a discontinuity error occurs, the router removes the sampling for that interval.
- mibId—Object ID of the discontinuity MIB attribute that you want to use for this trigger
- discontinuity-id-type—Specifies a discontinuity ID type (either timeStamp or timeTicks). The discontinuity ID type indicates the time value that you expect for a specific sample.

#### Mode

SNMP Trigger Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]