[Contents] [Prev] [Next] [Index] [Report an Error]

# ip unreachables

#### Syntax

[ no ] ip unreachables

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables the generation of an ICMP unreachable message when a packet is received that cannot be delivered by the router. The no version disables this function.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]