[Contents] [Prev] [Next] [Index] [Report an Error]

# Prefix Lists

A prefix list is a sequential collection of permit and deny conditions that apply to IP or IPv6 addresses. Like an access list, the router tests addresses one by one against the conditions in a prefix list. The first match determines whether the router accepts or rejects the address. Because the router stops testing conditions after the first match, the order of the conditions is critical. If no conditions match, the router rejects the address. An empty prefix list results in an automatic permit of the tested address.

Unlike access lists, the prefix list specifies a base IP or IPv6 address and a length (the number of bits applied to the base to determine the network prefix). The tested address is matched against the prefix.

Use the ip prefix-list command to define an IP prefix list, or the ipv6 prefix-list command to define an IPv6 prefix list. The prefix-list keyword with either the match { ip | ipv6 } address or match { ip | ipv6 } next-hop commands enables you to add a clause to a route map.

## Using a Prefix List

The following example creates a prefix list that permits routes with a prefix length up to 24 in the 151.0.0.0/8 network:

`

host1(config)#ip prefix-list abc permit 151.0.0.0/8 le 24

`

clear ip prefix-list

- Use to clear all hit counts in the prefix lists or the specified entry from the specified prefix list. (The router increments the hit count by 1 each time an entry matches.)
- Example
  `
  host1#clear ip prefix-list abc
  `
- There is no no version.
- See clear ip prefix-list.

clear ipv6 prefix-list

- Use to clear all hit counts in the IPv6 prefix lists or the specified entry from the specified prefix list. (The router increments the hit count by 1 each time an entry matches.)
- Example
  `
  host1#clear ipv6 prefix-list abc
  `
- There is no no version.
- See clear ipv6 prefix-list.

ip prefix-list

ipv6 prefix-list

- Use to create a prefix list for route filtering and to specify a list entry—a deny or permit clause for a network address—to the prefix list. Use to add entries to prefix lists.
- The prefix list name can be up to 32 characters long.
- Specify the position of each entry in the list with the seq (sequence) keyword. If you do not specify a sequence number, the router uses the value of the last sequence number plus 5.
- Use the ge and le keywords to specify a range of network prefixes. These keywords have the following values:
  - prefix length < ge <= 32
  - prefix length < le <= ge
- If you do not specify either the ge or le keyword, an exact match is expected.
- Example 1—IPv4; exact match required; the router permits only a route with a prefix length of 8 and a network address of 151.0.0.0.
  `
  host1(config)#ip prefix-list abc permit 151.0.0.0/8
  `
- Example 2—IPv6; exact match required; the router permits only a route with a prefix length of 8 and a network address of 1:0:0:0:0:0:0:5.
  `
  host1(config)#ipv6 prefix-list abc permit 1::5/8
  `
- Use the no version to remove the specified prefix list or the specified list entry.
- See ip prefix-list.
- See ipv6 prefix-list.

match ip address

- Use to specify an access list or use with the prefix-list or prefix-tree keyword to match routes that have a destination network number address that is permitted by any specified access list, prefix list, or prefix tree.
- Example
  `
  host1(config-route-map)#match ip address prefix-list abc
  `
- Use the no version to delete the match clause from a route map or a specified value from the match clause.
- See match ip address.

match ipv6 address

- Use to match any route that has a destination network number address that is permitted by the specified access list or prefix list.
- Example
  `
  host1(config-route-map)#match ipv6 address prefix-list boston
  `
- Use the no version to delete all address match clauses from a route map unless you specify an access list or prefix list, in which case only the list match is removed from the route map.
- See match ipv6 address.

match ip next-hop

- Use with the prefix-list keyword to match routes that have a next-hop router address passed by the specified access lists, prefix lists, or prefix trees.
- Example
  `
  host1(config-route-map)#match ip next-hop prefix-list abc
  `
- Use the no version to delete the match clause from a route map or a specified value from the match clause.
- See match ip next-hop.

match ipv6 next-hop

- Use to match any routes that have a next-hop router address passed by the specified access list or prefix list.
- Example
  `
  host1(config-route-map)#match ipv6 next-hop prefix-list next1
  `
- Use the no version to delete all next-hop match clauses from a route map unless you specify an access list or prefix list, in which case the router removes only the list match from the route map.
- See match ipv6 next-hop.

[Contents] [Prev] [Next] [Index] [Report an Error]