[Contents] [Prev] [Next] [Index] [Report an Error]

# show mpls rsvp bfd interfaces

#### Syntax

show mpls rsvp bfd interfaces [ filter ]

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Displays session information for RSVP-TE interfaces on which BFD is enabled, including minimum interval, minimum receive interval, minimum transmit interval, and multiplier values.

#### Options

- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]