[Contents] [Prev] [Next] [Index] [Report an Error]

## interModuleCommunication

#### Description

Intermodule communication monitoring

#### Emergency

None

#### Alert

None

#### Critical

Line module resetting after recovery attempts fail; standby SRP module resetting after monitoring thresholds exceeded; primary SRP module resetting after all line modules fail because of issue with primary SRP module

#### Error

None

#### Warning Log

Line module recovery attempts after monitoring thresholds exceeded

#### Notice Log

Ping monitoring threshold exceeded; ICC session monitoring threshold exceeded; ICC connection monitoring threshold exceeded

#### Info

Intermodule communication monitoring condition, state change, and corresponding action

#### Debug

None

#### Filter

slot slotNumber

- slot—Logs events for a specific slot
- slotNumber—Number of slot for which you want to log events

[Contents] [Prev] [Next] [Index] [Report an Error]