[Contents] [Prev] [Next] [Index] [Report an Error]

# atm framing

#### Syntax

atm framing framingType

no atm framing

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures T3 or E3 framing on an ATM interface. The no version returns framing to the default. For a T3 interface, the default value is cbitplcp. For an E3 interface, the default value is g751plcp.

#### Options

- framingType—One of the following:
  - cbitadm—c-bit with ATM direct mapping for a DS3 (T3) interface
  - cbitplcp—c-bit with PLCP framing for a DS3 (T3) interface (default for T3)
  - g832adm—G.832 ATM direct mapping for an E3 interface
  - g751adm—G.751 ATM direct mapping for an E3 interface
  - g751plcp—G.751 PLCP mapping for an E3 interface (default for E3)
  - m23adm—M23 ATM direct mapping for a DS3 (T3) interface
  - m23plcp—M23 with PLCP framing for a DS3 (T3)

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]