[Contents] [Prev] [Next] [Index] [Report an Error]

# Clearing BGP Attributes for VPLS

You can use the following clear ip bgp commands to remove specific BGP attributes for the L2VPN address family, and in one case, for the VPLS address family associated with a specific VPLS instance.

## Clearing BGP Reachability Information for the L2VPN Address Family

To clear BGP reachability information for the L2VPN address family:

- Issue the clear ip bgp command.
  `
  host1#clear ip bgp l2vpn soft in
  `

Use the soft in keywords to trigger inbound soft reconfiguration. There is no no version.

## Clearing BGP Route Flap Dampening Information for the L2VPN Address Family

To clear route flap dampening information for the L2VPN address family:

- Issue the clear ip bgp dampening command.
  `
  host1#clear ip bgp l2vpn dampening
  `

There is no no version.

## Clearing BGP Route Flap Dampening Information for the VPWS Address Family

To clear route flap dampening information for the VPLS address family associated with the specified VPLS instance:

- Issue the clear ip bgp dampening command.
  `
  host1#clear ip bgp vpls vplsA dampening
  `

There is no no version.

## Clearing the Wait for the End-of-RIB Marker for the L2VPN Address Family

To clear the wait for receiving an End-of-RIB marker from the peer for the L2VPN address family:

- Issue the clear ip bgp wait-end-of-rib command.

host1#clear ip bgp l2vpn wait-end-of-rib

#### Related Topics

- Configuring BGP Routing
- clear ip bgp
- clear ip bgp dampening
- clear ip bgp wait-end-of-rib

[Contents] [Prev] [Next] [Index] [Report an Error]