> - Download PDFs
> - show radius remote-circuit-id-format

> # show radius remote-circuit-id-format

> #### Syntax

> show radius remote-circuit-id-format

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays the format of the PPPoE remote circuit ID value sent from a DSLAM and captured on the router.

> If the PPPoE remote circuit ID value is configured to include any or all of the agent-circuit-id, agent-remote-id, and nas-identifier components, the display lists the components included and the order in which they appear.

> If the PPPoE remote circuit ID value is configured to use the format for the dsl-forum-1 keyword of the radius remote-circuit-id-format command, the display indicates that this format is in effect.

> #### Mode

> Privileged Exec

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.