[Contents] [Prev] [Next] [Index] [Report an Error]

# debounce-interval

#### Syntax

debounce-interval seconds

no debounce-interval

#### Release Information

Command introduced in JUNOSe Release 9.3.0.

#### Description

Modifies the minimum time an Ethernet interface must maintain a given state—for example, up or down—before the interface notifies the upper-layer protocols of the state change. The no version restores the default value, 1 second.

| Note: You can configure this command only if you have enabled the debounce timer feature using the debounce command.

#### Options

- seconds—Interval for which an interface must maintain a given state before the interface reports the state change to the upper-layer protocols. Number in the range 1–5 seconds; default value is 1 second.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]