[Contents] [Prev] [Next] [Index] [Report an Error]

# slot accept

#### Syntax

slot accept slotNum [ subsystem ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Erases from NVS the type and configuration of the previous module in the specified slot, and allows you to configure a new module. Issue this command after you have installed a different type of module in a slot. You can use this command only when the state of the module in the slot is not present or disabled (mismatch). There is no no version.

#### Options

- slotNum—For ERX7xx models, a number in the range 0–6; for ERX14xx models, a number in the range 0–13; for the ERX310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16
- subsystem—Type of subsystem on the E120 and E320 routers; use when the specified slotNumber is a slot that contains an SRP module
  - srp—Indicates the SC on one or both SRP modules; specify this keyword to accept only the configuration of the portion of the SC on the individual SRP module
  - fabric—Indicates the portion of the switch fabric on the SRP modules; specify this keyword to accept only the configuration of an individual fabric slice

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]