[Contents] [Prev] [Next] [Index] [Report an Error]

# Router Power Requirements

Table 16 lists the maximum power requirements for various components in an E120 router or E320 router when the router is operating under typical voltage conditions.

Table 16: Power Requirements for E120 Router and E320 Router

Component | Watts | Amps@48V
--- | --- | ---
E320 Fan Tray | 460 | 9.58
E120 Fan Tray | 108 | 2.25
SRP IOA | 10 | 0.21
SRP-100 | 75 | 1.56
SFM-100 | 40 | 0.83
SRP-120 | 140 | 2.92
SFM-120 | 95 | 1.98
SRP-320 | 140 | 2.92
SFM-320 | 95 | 1.98
ES2 4G LM | 176 | 3.67
ES2 10G UPLINK LM | 150 | 3.13
ES2 10G LM | 198 | 4.13
ES2 10G ADV LM | 190 | 4.0
ES2-S1 GE-4 IOA | 18 | 0.38
ES2-S1 GE-8 IOA | 21 | 0.44
ES2-S3 GE-20 IOA | 92 | 1.92
ES2-S1 10GE IOA | 40 | 0.83
ES2-S1 OC3-8 ATM IOA | 50 | 1.04
ES2-S1 OC12-2 ATM IOA | 40 | 0.83
ES2-S1 OC12-2 POS IOA | 30 | 0.63
ES2-S1-OC48 POS IOA | 30 | 0.63
ES2-S1 REDUND IOA | 10 | 0.21
ES2-S1 SERVICE IOA | 10 | 0.21

[Contents] [Prev] [Next] [Index] [Report an Error]