[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Statistics about the RADIUS Route-Download Server

#### Purpose

Display statistics about the RADIUS route-download server configuration.

- Use the optional statistics keyword to display information about the RADIUS route download server operation.
- Use the optional delta keyword to show baselined statistics.

#### Action

To display statistics about the RADIUS route-download server configuration:

    host1#show aaa route-download
    AAA Route Downloader:     configured in virtual router default
    Download Interval:        720 minutes
    Retry Interval:           10 minutes
    Default Cost:             2
    Default Tag:              0
    Base User Name:           <HOSTNAME>
    Password:                 <DEFAULT>
    Synchronization:          <NOT SET>

    Status:                   idle
    Last Download Attempt:    TUE DEC 19 22:46:47 2006
    Last Download Success:    TUE DEC 19 22:46:47 2006
    Last Regular Download:    complete
    Next Download Scheduled:  WED DEC 20 10:46:47 2006
    Next Regular Download:    WED DEC 20 10:46:47 2006

To display information about the RADIUS route download server operation:

    host1#show aaa route-download statistics

    Total Download Attempts: 2
    Successful Downloads:    2
    Downloaded Fragments:    3756
    Downloaded Routes:       192000
    IP Updates:              1
    Updated Routes:          96000
    Cleared Route Intervals: 0

#### Meaning

Table 14 lists the show aaa route-download command output fields.

Table 14: show aaa route-download Output Fields

Field Name | Field Description
--- | ---
AAA Route Downloader | Virtual router where the RADIUS route-download server is configured
Download Interval | Number of minutes between route downloads
Retry Interval | Number of minutes before retry after a download failure
Default Cost | Default cost of downloaded routes
Default Tag | Default tag for downloaded routes
Base User Name | Virtual router used for route-download requests; either <HOSTNAME> or the configured name
Password | Password for route-download requests or <DEFAULT>
Synchronization | Either <NOT SET> or the time that the server starts the route download operation each day
Status | Current status of route-download server; waiting for base router, waiting for IP warmstart, idle, downloading, updating ip, downloading and updating ip, or suspended
Last Download Attempt | Either <NEVER> or the day, date, and time of attempt
Last Download Success | Either <NEVER> or the day, date, and time of success
Last Regular Download | Status of last regular download; either complete or not complete
Next Download Scheduled | <DOWNLOAD ACTIVE>,<NOT SCHEDULED>, or the day, date, and time of next download
Next Regular Download | Day, date, and time
Total Download Attempts | Number of downloads attempted
Successful Downloads | Number of successful download operations
Downloaded Fragments | Number of downloaded fragments
Downloaded Routes | Number of downloaded routes
IP Updates | Number of IP updates
Updated Routes | Number of updated routes
Cleared Route Intervals | Number of cleared route intervals

#### Related Topics

- show aaa route-download

[Contents] [Prev] [Next] [Index] [Report an Error]