> - radius override calling-station-id remote-circuit-id

> # radius override calling-station-id remote-circuit-id

> #### Syntax

> radius override calling-station-id remote-circuit-id

> no radius override calling-station-id

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures RADIUS to override the standard use of the Calling-Station-Id [31] RADIUS attribute and instead use the PPPoE remote circuit ID transmitted from a DSLAM device. The no version restores the default Calling-Station-Id value, which is the telephone number from which the call originated.

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.