[Contents] [Prev] [Next] [Report an Error]

# OC12/STM4 POS Single-Mode Intermediate Reach With APS/MSP Redundancy Module Combination

> Line module label | OCx/STMx POS
> I/O module label | OC12 STM4 APS SINGLE MODE
> Number of I/O ports | 1 active, 1 redundant
> Software release | First supported: 2.0.0 Final supported: Not applicable
> Description | 120 W Unchannelized, concatenated OC12/STM4 for POS
> Type | EFA ASIC
> Capability | OC12/STM4 HDLC framing
> Software features | See OCx/STMx POS and OC48 Modules for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX7xx models ERX14xx models ERX310 router
> SRP module compatibility | SRP-5G+ SRP-10G SRP-40G SRP-40G PLUS SRP-SE10G
> Module redundancy support | 1:N redundancy NOTE: Line module redundancy is not supported on the ERX310 router.
> Cables and connectors | SC full duplex Tx power: min: –15 dBm max: –8 dBm Center wavelength: 1310 nm Rx input power: min: –31 dBm max: –8 dBm Rated for 15 km (9.3 miles) of 9-micron core cable See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See Module LEDs.
> Alarms, errors, and events | See Monitoring SONET/SDH Interfaces in JUNOSe Physical Layer Configuration Guide, Chapter 3, Configuring Unchannelized OCx/STMx Interfaces.

[Contents] [Prev] [Next] [Report an Error]