[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Configuration of Tunnel Parameters with AAA

#### Purpose

Display configuration of tunnel parameters used for tunnel definitions.

#### Action

To display the configuration of tunnel parameters used for tunnel definitions:

    host1#show aaa tunnel-parameters
    Tunnel password is 3&92k%b#q4
    Tunnel client-name is <NULL>
    Tunnel nas-port-method is none
    Tunnel switch profile is boston
    Tunnel tx-connect-speed-method is qos
    Tunnel nas-port ignore disabled
    Tunnel nas-port-type ignore disabled
    Tunnel assignmentId format is assignmentId
    Tunnel calling number format is fixed (stacked)
     Tunnel calling number format fallback is fixed

#### Meaning

Table 81 lists the show aaa tunnel-parameters command output fields.

Table 81: show aaa tunnel-parameters Output Fields

Field Name | Field Description
--- | ---
Tunnel password | Default tunnel password
Tunnel client-name | Hostname that the LAC sends to the LNS when communicating about the tunnel
Tunnel nas-port-method | Default NAS port type
Tunnel switch profile is | Name of the default L2TP tunnel switch profile
Tunnel tx-connect-speed-method is | Method that the router uses to calculate the transmit connect speed of the subscriber’s access interface: static layer2, dynamic layer2, qos, actual, not set
Tunnel nas-port ignore | Whether the router uses the tunnel peer’s NAS-Port [5] attribute; enabled or disabled
Tunnel nas-port-type ignore | Whether the router uses the tunnel peer’s NAS-Port-Type [61] attribute; enabled or disabled
Tunnel assignmentId format | Value of the tunnel assignment ID that is passed to PPP/L2TP
Tunnel calling number format | Format configured for L2TP Calling Number AVP 22 generated by the LAC
Tunnel calling number format fallback | Fallback format configured for L2TP Calling Number AVP 22 generated by the LAC

#### Related Topics

- show aaa tunnel-parameters

[Contents] [Prev] [Next] [Index] [Report an Error]