[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls spf-use-any-best-path

#### Syntax

[ no ] mpls spf-use-any-best-path

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables the SPF calculations to consider both the best IGP (IS-IS or OSPF) paths and the MPLS tunnel to reach the tunnel endpoint. The no version restores the default value, which is to always use the MPLS tunnel to reach the tunnel endpoint—the IGP best paths are not considered.

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]