[Contents] [Prev] [Next] [Index] [Report an Error]

# Using the Null Interface

You can use access control lists to filter undesired traffic. Another way to handle undesired traffic is to send it to the null interface. The router automatically creates the null interface, which is always up, cannot be deleted, and acts as a data sink. In other words, the null interface cannot forward or receive traffic. However, the CLI does allow you to access the null interface.

The E Series router creates the null interface by default; you do not have to manually create it. You can direct traffic to the null interface by specifying the null 0 keywords instead of a next-hop or destination address when you configure routes.

interface null

- Use to access the null interface.
- The null interface is a data sink; it does not accept or forward traffic.
- Although you can access the null interface, you cannot configure any values for it or delete it.
- Example
  `
  host1(config)#interface null 0
  host1(config-if)#
  `
- There is no no version.
- See interface null.

ip route

- Use to configure a static route and redirect traffic from it to the null interface.
- Example
  `
  host1(config-if)#ip route 10.10.20.5 null 0
  `
- Use the no version to remove the static route.
- See ip route.

[Contents] [Prev] [Next] [Index] [Report an Error]