[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls traffic-eng

#### Syntax

mpls traffic-eng level-1 | level-2

no mpls traffic-eng level-1 | level-2

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables flooding of MPLS traffic-engineering link information into the specified IS-IS level. Flooding is disabled by default. The no version disables flooding.

#### Options

- level-1—Floods IS-IS level 1
- level-2—Floods IS-IS level 2

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]