[Contents] [Prev] [Next] [Index] [Report an Error]

# Powering Up

For specifications on the electrical requirements for the system, see System Specifications. For details on the power consumed by the different ERX modules, see the ERX Module Guide.

| Note: In this procedure, we assume that the system is already connected to a power source. See Cabling ERX Routers.

| Caution: Evaluate the overall loading of the branch circuit before you install any equipment into a rack.

To power up the system:

1. Verify that the power source is operational and turned on.
2. Inspect all grounding and power connections to the router chassis.
3. Confirm that all connections are secure.
4. Switch the power switches to ON.
5. Monitor the LEDs on the front of the SRP modules to verify that the system is booting properly. See Table 11 in Troubleshooting for LED status explanations.

   When the prompt appears on the system console, the system is in User Exec mode and is ready to be configured:

   `
   host1>
   `
6. Enter the enable command to access Privileged Exec mode:
   `
   host1>enable
   host1#
   `

   In Privileged Exec mode you can begin to configure the system. See JUNOSe System Basics Configuration Guide, Chapter 2, Command-Line Interface for more information.

## Initialization Sequence

Each line module is initialized independently. As a result, the CLI on the SRP module can become available before the line modules have completed initialization. Commands relating to a line module might fail if the module has not completed initialization. You can use the show version command to display line module status. Do not enter commands for a line module until its state is listed as online.

[Contents] [Prev] [Next] [Index] [Report an Error]