[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Secure CLACL Configurations

#### Purpose

Display information about only secure CLACL configurations. This command and the output are visible only to authorized users—the mirror-enable command must be enabled before using this command. Use the brief or detail keywords with the show secure classifier-list command to display different levels of information.

#### Action

To display a list of secure CLACLs

    host1#show secure classifier-list

                             Classifier Control List Table
                             ---------- ------- ---- -----
    Secure IP secClassA.1 ip any any
    Secure IP secClassB.1 ip any not 10.10.10.1 255.255.255.255
    Secure IP secClass25.1 user-packet-class 8 source-route-class 100 ip
    192.168.44.103 255.255.255.255 any

Displays details of each secure CLACL

    host1#show secure classifier-list secClass25 detailed

                             Classifier Control List Table
                             ---------- ------- ---- -----
    Secure IP Classifier Control List secClass25
       Reference count:      0
       Entry count:          1

       Classifier-List secClass25 Entry 1
          User Packet Class:          8
          Source Route Class:         100
          Protocol:                   ip
          Not Protocol:               false
          Source IP Address:          192.168.44.103
          Source IP WildcardMask:     255.255.255.255
          Not Source Ip Address:      false
          Destination IP Address:     0.0.0.0
          Destination IP WildcardMask:255.255.255.255
          Not Destination Ip Address: false

#### Meaning

Table 66 lists show secure classifier-list command output fields.

Table 66: show secure classifier-list Output Fields

Field Name | Field Description
--- | ---
Reference count | Number of times the CLACL is referenced by policies
Entry count | Number of entries in the classifier list
Classifier-List | Name of the classifier list
Entry | Entry number of the classifier list rule
Color | Packet color to match: green, yellow, or red
Protocol | Protocol type
Not Protocol | If true, matches any protocol except the preceding protocol; if false, matches the preceding protocol
Source IP Address | Address of the network or host from which the packet is sent
Source IP WildcardMask | Mask that indicates addresses to be matched when specific bits are set
Not Source Ip Address | If true, matches any source IP address and mask except the preceding source IP address and mask; if false, matches the preceding source IP address and mask
Destination IP Address | Number of the network or host from which the packet is sent
Destination IP WildcardMask | Mask that indicates addresses to be matched when specific bits are set
Not Destination Ip Address | If true, matches any destination IP address and mask except the preceding destination IP address and mask; if false, matches the preceding destination IP address and mask
Traffic Class | Name of the traffic class to match
User Packet Class | User packet value to match
DS Field | DS field value to match
TOS Byte | ToS value to match
Precedence | Precedence value to match
User Priority bits | User priority bits value to match
Traffic Class Field | Traffic class field value to match
EXP Bits | MPLS EXP bit value to match
EXP Mask | Mask applied to EXP bits before matching
DE Bit | Frame Relay DE bit value to match5.2.0b1 ID-1381
Destination Route Class | Route class used to classify packets based on the packet’s destination address
Source Route Class | Route class used to classify packets based on the packet’s source address
Local | If true, matches packets destined to a local interface; if false, matches packets that are traversing the router

#### Related Topics

- show secure classifier-list

[Contents] [Prev] [Next] [Index] [Report an Error]