[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Upper-Layer Dynamic Interfaces and Profiles

You can use the show commands described in this section to monitor configurations created with dynamic interfaces and profiles.

| Note: The E120 and E320 routers output for monitor and show commands is identical to output from other E Series routers, except that the E120 and E320 routers output also includes information about the adapter identifier in the interface specifier (slot/adapter/port).

show atm aal5 interface

- Use to display information about a configured ATM AAL5 interface.
- Field descriptions
  - AAL5 Interface operational status—Operational status of the AAL5 interface: up, down, lowerLayerDown
  - time since last status change—Time since last reported change to the AAL5 interface operational status in hh:mm:ss format
  - SNMP trap link-status—Whether SNMP link status traps are enabled or disabled on the ATM AAL5 interface
  - Auto configure ATM 1483 status—Whether the autoconfiguration feature for a dynamic ATM 1483 subinterface configured over the ATM AAL5 interface is enabled or disabled
  - InPackets—Number of packets received on this interface
  - InBytes—Number of bytes received on this interface
  - OutPackets—Number of packets transmitted on this interface
  - OutBytes—Number of bytes transmitted on this interface
  - InErrors—Number of incoming errors received on this interface
  - OutErrors—Number of outgoing errors on this interface
  - InPacketDiscards—Number of incoming packets discarded on this interface
  - OutDiscards—Number of outgoing packets discarded on this interface
- Example

      host1#show atm aal5 interface atm 3/0
      AAL5 Interface ATM 3/0 operational status:    lowerLayerDown
            time since last status change: 00:08:46

      SNMP trap link-status: disabled
      Auto configure ATM 1483 status: disabled

      InPackets:        0
      InBytes:          0
      OutPackets:       0
      OutBytes:         0
      InErrors:         0
      OutErrors:        0
      InPacketDiscards: 0
      OutDiscards:      0

- See show atm aal5 interface.

show atm subinterface

- Use to display the current state of all ATM subinterfaces, all ATM subinterfaces configured on a specified ATM physical interface, or a specific ATM subinterface.
- To specify an ATM subinterface for ERX7xx models, ERX14xx models, and ERX310 router, use the slot/port.subinterface format.
  - slot—Number of the chassis slot
  - port—Port number on the I/O module
  - subinterface—Number of the subinterface in the range 1–2147483647
- To specify an ATM subinterface for E120 and E320 routers, use the slot/adapter/port.subinterface format.
  - slot—Number of the chassis slot
  - adapter—Identifier for the IOA within the E320 chassis, either 0 or 1, where:
    - 0 indicates that the IOA is installed in the right IOA bay (E120 router) or the upper IOA bay (E320 router).
    - 1 indicates that the IOA is installed in the left IOA bay (E120 router) or the lower IOA bay (E320 router).
  - port—Port number on the IOA
  - subinterface—Number of the subinterface in the range 1–2147483647
- To display brief summary information for all ATM subinterfaces, or for ATM subinterfaces configured on a specified ATM physical interface, use the summary keyword.
- To display status information only for ATM subinterfaces with a specific operating status, use the status keyword with one of the following status values. (See the Status field description for an explanation of these values.)
  - dormant
  - dormantLockout
  - down
  - lowerLayerDown
  - notPresent
  - up
- To display the current state of an ATM subinterface created on the PVC with the specified VPI and VCI values, use the atm slot/port/vpi/vci format (for ERX7xx models, ERX14xx models, and ERX310 router) or the slot/adapter/port/vpi/vci format (for E120 and E320 routers) to identify the ATM subinterface (Example 5).

  | Note: You can use the atm slot/port/vpi/vci format as an alternative to the atm slot/port.subinterface format with the specific show interface and show subinterface commands to monitor all ATM 1483 subinterfaces (except NBMA interfaces) as well as the upper-layer interfaces configured over an ATM 1483 subinterface. You cannot, however, use the atm slot/port/vpi/vci format to create or modify an ATM 1483 subinterface. These guidelines also apply to E120 and E320 routers when you use the atm slot/adapter/port/vpi/vci format as an alternative to the atm slot/adapter/port.subinterface format.

- For more information, see Creating a Basic Configuration in Configuring ATM .
- Field descriptions
  - Interface—Interface identifier
  - ATM-Prot—One of the following ATM protocol types:
    - RFC-1483—Multiprotocol encapsulation over AAL5
    - NBMA—Nonbroadcast multiaccess interface
    - ATM/MPLS—Local ATM passthrough interface
  - VCD—Virtual circuit descriptor
  - VPI—Virtual path identifier
  - VCI—Virtual circuit (or channel) identifier
  - Circuit Type—Type of circuit: PVC
  - Encap—Administered encapsulation method based on what was configured with the atm pvc command
  - MTU—Maximum transmission unit size for the interface
  - Status—One of the following ATM 1483 subinterface states:
    - absent—Represents the notPresent state and indicates that, although the SRP detects the ATM 1483 subinterface, the module on which the subinterface resides has not completed booting up, has failed, or is disabled.
    - dormant—Indicates that the ATM 1483 subinterface is performing autodetection of one or more upper-layer encapsulation types and is waiting to receive a packet of that type on a lower-layer interface. An ATM 1483 subinterface transitions from the dormant state to the up state when the router receives a valid packet of the specified encapsulation type on the interface.
    - dormantLockout—Indicates that a dormant ATM 1483 subinterface has one or more upper-layer encapsulation types currently undergoing encapsulation type lockout. An ATM 1483 subinterface transitions from the dormantLockout state to the dormant state when the lockout time expires for all upper-layer encapsulation types undergoing lockout. An ATM 1483 subinterface transitions from the dormantLockout state to the up state when the router receives a valid packet for an encapsulation type that is configured for autodetection but is not undergoing lockout.
    - down—Indicates that the ATM 1483 subinterface is administratively disabled or has a circuit that is down or not configured.
    - lowerLayerDown—Indicates that a lower-layer interface below the ATM 1483 subinterface is down.
    - up—Indicates that the ATM 1483 subinterface is up and able to transfer data. For an ATM 1483 subinterface that supports one or more dynamic upper-layer interfaces, indicates that the router has created the dynamic upper-layer interface or is in the process of creating it.
  - Interface Type—Type of ATM 1483 subinterface: dynamic or static
  - Auto configure status—Setting of the autoconfiguration feature
    - dynamic—Autodetection is on; the router automatically detects the next upper interface
    - static—Autodetection is off
  - Auto configure interface(s)—Types of dynamic upper interfaces configured with the auto-configure command: bridged Ethernet, IP, PPP, or PPPoE
  - Detected 1483 encapsulation—If the encapsulation type is set to aal5autoconfig, displays the 1483 encapsulation type detected on the subinterface (displays AUTO until a packet is detected)
  - Detected dynamic interface—Type of dynamic upper interface detected during autoconfiguration: bridged Ethernet, IP, PPP, PPPoE, or (if no packet has been received) none
  - Interface types in lockout—Encapsulation types currently experiencing lockout: bridged Ethernet, IP, PPP, PPPoE, or none
  - Lockout state (seconds)—Settings of encapsulation type lockout for the upper-layer encapsulation type indicated
    - Min—Minimum lockout time, in seconds
    - Max—Maximum lockout time, in seconds
    - Current—Current lockout time, in seconds; displays 0 (zero) if lockout is not occurring
    - Elapsed—Time elapsed into the lockout time, in seconds; displays 0 (zero) if lockout is not occurring
    - Next—Lockout time for the router to use for the next lockout event, in seconds
  - Assigned profile—For each dynamic interface type, indicates whether or not a profile is assigned and, if assigned, displays the profile name
  - Subscriber info—Subscriber login information for the specified dynamic interface type (bridged Ethernet or IP)
  - SNMP trap link-status—Trap link status: enabled or disabled
  - InPackets—Number of packets received on this interface
  - InBytes—Number of bytes received on this interface
  - OutPackets—Number of packets transmitted on this interface
  - OutBytes—Number of bytes transmitted on this interface
  - InErrors—Number of errors received on this interface
  - OutErrors—Number of outgoing errors on this interface
  - InPacketDiscards—Number of incoming packets discarded on this interface
  - InPacketsUnknownProtocol—Number of incoming packets with an unknown protocol type
  - OutDiscards—Number of outgoing packets discarded on this interface
- Example 1—Displays the current state of all ATM subinterfaces

      host1#show atm subinterface
                                      Circuit                         Interface
      Interface   ATM-Prot VCD VPI VCI Type  Encap MTU    Status      Type
      ----------- -------- --- --- --- ----- ----- ---- ----------- -------
      ATM 2/0.101 RFC-1483 101   0 101 PVC   AUTO  9180 dormantLockout Static
      ATM 2/0.102 RFC-1483 102   0 102 PVC   AUTO  9180 up             Dynamic
      ATM 2/0.103 RFC-1483 103   0 103 PVC   AUTO  9180 dormant        Static
      3 interface(s) found

- Example 2—Displays summary information for all ATM subinterfaces shown in Example 1

      host1#show atm subinterface summary
      3 subinterfaces: 1 up, 0 down,
      1 dormant, 1 dormantLockout,
      0 lowerLayerDown, 0 not present

- Example 3—Displays status information for all ATM subinterfaces in the dormantLockout state

      host1#show atm subinterface status dormantLockout
                                      Circuit                        Interface
       Interface  ATM-Prot VCD VPI VCI  Type Encap MTU  Status       Type
      ---------- -------- --- --- --- ------ ----- ---- ------------- ---------
      ATM 2/0.101 RFC-1483 101   0 101 PVC   AUTO  9180 dormantLockout Static
      1 interface(s) found

- Example 4—Displays the current state of a specific ATM subinterface

      host1#show atm subinterface atm 2/0.101
                                      Circuit                        Interface
       Interface  ATM-Prot VCD VPI VCI Type Encap MTU    Status      Type
      ----------- -------- --- --- --- ----- ----- ---- ------------ ---------
      ATM 2/0.101 RFC-1483 101  0 101 PVC   AUTO  9180 dormantLockout Static

      Auto configure status         : dynamic
      Auto configure interface(s)   : IP  bridgedEthernet  PPP  PPPoE
      Detected 1483 encapsulation   : AUTO
      Detected dynamic interface    : none
      Interface types in lockout    : IP

      Lockout state (seconds)       : Min Max  Current Elapsed Next
      ------------------------------- --- ---- ------- ------- ----
      IP                                1   30      16       7   30
      BridgedEnet                     900 3600       0       0  900
      PPP                               1  300       0       0    1
      PPPoE                             1  300       0       0    1

      Assigned profile (IP)         : ipoa
      Assigned profile (BridgedEnet): beth
      Assigned profile (PPP)        : ppptest
      Assigned profile (PPPoE)      : pppoetest
      Assigned profile (any)        : none assigned

      BridgedEnet subscriber info   :
      Username: elaine@jpeterman.com
      Password: putty
      Authenticate: enabled

      SNMP trap link-status: disabled

      InPackets:                0
      InBytes:                  1904
      OutPackets:               0
      OutBytes:                 0
      InErrors:                 0
      OutErrors:                0
      InPacketDiscards:         14
      InPacketsUnknownProtocol: 0
      OutDiscards:              0
      1 interface(s) found

- Example 5—Displays the current state of a specific ATM subinterface created on the PVC with the specified VPI and VCI values

      host1#show atm subinterface atm 0/0/0/101
                                       Circuit                   Interface
       Interface  ATM-Prot VCD VPI VCI  Type   Encap MTU  Status   Type
      ----------- -------- --- --- --- ------- ----- ---- ------ ---------
      ATM 0/0.101 RFC-1483 101   0 101 PVC     AUTO  9180 up     Static

      Auto configure status         : dynamic
      Auto configure interface(s)   : PPPoE
      Detected 1483 encapsulation   : SNAP
      Detected dynamic interface    : PPPoE
      Interface types in lockout    : none

      Lockout state (seconds)       : Min Max Current Elapsed Next
      ------------------------------- --- --- ------- ------- ----
      PPPoE                             1 300       0       0    1

      Assigned profile (IP)         : none assigned
      Assigned profile (BridgedEnet): none assigned
      Assigned profile (PPP)        : none assigned
      Assigned profile (PPPoE)      : pppoeprofile
      Assigned profile (any)        : none assigned

      SNMP trap link-status: disabled

      InPackets:                5119
      InBytes:                  358672
      OutPackets:               5107
      OutBytes:                 357510
      InErrors:                 0
      OutErrors:                0
      InPacketDiscards:         3
      InPacketsUnknownProtocol: 0
      OutDiscards:              0
      1 interface(s) found

- See show atm subinterface.

show atm vc

- Use to display a summary of all configured ATM VCs and reserved VC ranges.
- You can specify one or more of the following keywords individually or in combination:
  - vpi—Displays VCs on a specific VPI
  - category—Displays VCs that have a specific service category
  - status—Displays VCs with a certain status
- To display only a summary of all reserved VC ranges on the router, specify the reserved keyword with no other keywords. This includes VPI/VCI ranges reserved for use by dynamic ATM 1483 subinterfaces.
- Field descriptions
  - Interface—Interface identifier
  - VPI—Virtual path identifier
  - VCI—Virtual channel identifier
  - VCD—Virtual circuit descriptor
  - Type—Type of circuit: PVC
  - Encap—Encapsulation method: AUTO, AAL5, MUX, SNAP, ILMI, F4-OAM
  - Category—Service type configured on the VC: UBR, UBR-PCR, NRT-VBR, RT-VBR, or CBR
  - Rx/Tx Peak—Peak rate, in Kbps
  - Rx/Tx Avg—Average rate, in Kbps
  - Rx/Tx Burst—Maximum number of cells that can be burst at the peak cell rate
  - Status—State of the virtual circuit: Up or Down
  - Start VPI—Starting virtual path identifier (inclusive) of the reserved VC range
  - Start VCI—Starting virtual circuit identifier (inclusive) of the reserved VC range
  - End VPI—Ending virtual path identifier (inclusive) of the reserved VC range
  - End VCI—Ending virtual circuit identifier (inclusive) of the reserved VC range
- Example 1—Displays all VCs and reserved VC ranges on the router

      host1#show atm vc
                                            Cate Rx/Tx Rx/Tx Rx/Tx Sta
      Interface    VPI VCI  VCD  Type Encap gory Peak   Avg  Burst tus
      ------------ --- ---- ---- ---- ----- ---- ----- ----- ----- ---
      ATM 3/0.2      0 101  4375 PVC  AUTO  CBR   1000     0     0 UP
      ATM 3/0.3      0 102  4376 PVC  AUTO  CBR   1000     0     0 DOWN
      ...
      ATM 3/0.8099   1 8099 8099 PVC  SNAP  UBR      0     0     0 UP
      ATM 3/0.8100   1 8100 8100 PVC  SNAP  UBR      0     0     0 DOWN
      8000 circuit(s) found

      Reserved VCC ranges:

                Start Start End End
      Interface  VPI   VCI  VPI VCI
      --------- ----- ----- --- ---
      ATM 2/0       2   100   2 102
      ATM 2/0       3   300   3 303
      2 reservation(s) found

- Example 2—Displays all reserved VC ranges on the router

      host1#show atm vc reserved
      Reserved VCC ranges:

                Start Start End End
      Interface  VPI   VCI  VPI VCI
      --------- ----- ----- --- ---
      ATM 2/0       2   100   2 102
      ATM 2/0       3   300   3 303
      2 reservation(s) found

- See show atm vc.

show columns

- Use to display static and dynamic interface counts for each interface column.
- Counts for PPP and PPPoE interface columns are updated when the PPP layer comes up.
- Counts for bridged Ethernet and IP over ATM columns are updated when the ATM layer comes up.
- Field descriptions
  - Type—Interface type
  - Total—Total number of interfaces on this column
  - Static—Number of static interfaces on this column
  - Dynamic—Number of dynamic interfaces on this column
- Example

      host#show columns
                        Interface columns:
                        ------------------
              Type           Total      Static    Dynamic
      -------------------- ---------- ---------- ----------
      Bridged Ethernet              4          2          2
      IP over ATM                   4          2          2
      PPP                          22         12         10
      PPPoE                        10          5          5

- See show columns.

show pppoe interface

- Use to display summary information about the encapsulation type lockout parameters configured for PPPoE clients on a dynamic PPPoE subinterface column.
- The following field descriptions and example include only the portion of the show pppoe interface command display relevant to lockout configuration for PPPoE clients. For more information about using this command, see show pppoe interface in Configuring Point-to-Point Protocol over Ethernet.
- Field descriptions
  - Lockout Configuration (seconds)—Encapsulation type lockout settings for the PPPoE client associated with the dynamic PPPoE subinterface column
    - Min—Minimum lockout time, in seconds
    - Max—Maximum lockout time, in seconds
    - Total clients in active lockouts—Number of PPPoE clients currently undergoing dynamic encapsulation type lockout
    - Total clients in lockout grace period—Number of PPPoE clients currently in a lockout grace period; for more information about the lockout grace period, see Guidelines for Configuring Encapsulation Type Lockout
- Example

      host1#show pppoe interface atm 3/0.101
      . . .
      Lockout Configuration (seconds): Min 5, Max 60
       Total clients in active lockouts: 0
       Total clients in lockout grace period: 0

- See show pppoe interface.

show pppoe interface lockout-time

- Use to display detailed information about the current encapsulation type lockout condition for each PPPoE client associated with a dynamic PPPoE subinterface column on a static PPPoE major interface.
- Field descriptions
  - PPPoE interface—Specifier for the PPPoE interface
  - Lockout Configuration (seconds)—Encapsulation type lockout settings for the PPPoE client associated with the dynamic PPPoE subinterface column
    - Min—Minimum lockout time, in seconds
    - Max—Maximum lockout time, in seconds
    - Total clients in active lockouts—Number of PPPoE clients currently undergoing dynamic encapsulation type lockout
    - Total clients in lockout grace period—Number of PPPoE clients currently in a lockout grace period; for more information about the lockout grace period, see Guidelines for Configuring Encapsulation Type Lockout
  - Client Address—Source MAC address of the PPPoE client
  - Current—Current lockout time, in seconds; displays 0 (zero) if the PPPoE client is not undergoing lockout
  - Elapsed—Time elapsed into the lockout time, in seconds; displays 0 (zero) if the PPPoE client is not undergoing lockout
  - Next—Lockout time that the router uses for the next lockout event, in seconds
- Example

      host1#show pppoe interface atm 3/0.101 lockout-time
      PPPoE interface ATM 3/0.101
      Lockout Configuration (seconds): Min 5, Max 60
       Total clients in active lockout: 0
       Total clients in lockout grace period: 0
      Client Address Current Elapsed Next
      -------------- ------- ------- ----
      0090.1a10.165e       0       0    5

- See show pppoe interface lockout-time.

show pppoe subinterface

- Use to display the source MAC address of a PPPoE client when a subscriber is connected to the router through an available PPPoE session. You can then specify this MAC address in pppoe clear lockout interface to clear the lockout condition for the PPPoE client.
- To display configuration, status, and statistics information, including the source MAC address of the PPPoE client, use the full keyword.
- The following field descriptions and example include only the portion of the show pppoe subinterface command display relevant to the source MAC address for PPPoE clients. For more information about using this command, see show pppoe subinterface in Configuring Point-to-Point Protocol over Ethernet.
- Field descriptions
  - PPPoE subinterface—Specifier for the PPPoE subinterface
  - source MAC address—MAC address of the PPPoE client associated with the dynamic PPPoE subinterface column
- Example

      host1#show pppoe subinterface full
      ...
          PPPoE subinterface ATM 3/0.101 has source MAC address 0090.1a10.165e
      ...

- See show pppoe subinterface.

show profile

- Use to display information about profiles.
- To display information about a specific profile, use the name keyword.
- To display a list of profiles configured on the router, use the brief keyword.
- Field descriptions
  - Profile—Name of the profile that is displayed
  - IP address—IP address and subnet mask of the interface, or none if the interface is unnumbered
  - Unnumbered interface—Specifier for the unnumbered interface, or none if the interface is numbered
  - Router—Name of the virtual router (VR) assigned to the profile; interfaces created by the profile are attached to this VR
  - Directed Broadcast—Enabled or disabled
  - ICMP Redirects—Enabled or disabled
  - Access Route Addition—Enabled or disabled
  - Network Address Translation—Enabled or disabled; domain location (inside or outside)
  - Source-Address Validation—Enabled or disabled
  - Ignore DF Bit—Enabled or disabled
  - Filter Option Packets—Router filters out packets with IP options; enabled or disabled
  - Administrative MTU—MTU size configured on the profile
  - TCP MSS value—Maximum segment size for TCP SYN packets traveling through the interface
  - Inactivity Timer—Inactivity timer setting; enabled or disabled
  - Route Map Name—Route map applied to the IP interface subscriber; enabled or disabled
  - Auto Detect—Router automatically detects packets that do not match any entries in the demultiplexer table; enabled or disabled
  - Auto Configure—Dynamic creation of subscriber interfaces on a primary IP interface; enabled or disabled
  - IGMP—Enabled or disabled
  - static-groups—Displays address of any static groups configured for IGMP
  - Input policy—Name of input policy and whether statistics are enabled or disabled
  - Output policy—Name of output policy and whether statistics are enabled or disabled
  - PPP Keepalive—PPP keepalive period, in seconds
  - PPP Magic Number—Enabled or disabled
  - PPP Magic Number Mismatch—Indicates whether the router is configured to ignore the LCP peer magic number and retain the PPP connection when the peer has not negotiated an LCP magic number: ignore (ignore the peer magic number mismatch and retain the PPP connection), or reject (router terminates the PPP connection if it detects a peer magic number mismatch)
  - PPP Peer DNS Priority—Enabled or disabled
  - PPP Peer WINS Priority—Enabled or disabled
  - PPP Authentication—Type of authentication configured: PAP, CHAP, or none
  - PPP Authentication Router—Name of authentication virtual router
  - PPP Negotiate MRU—MRU configured for the profile
  - PPP Packet Log—Enabled or disabled
  - PPP State Log—Enabled or disabled
  - PPP Chap Challenge Length—Minimum and maximum Chap Challenge length
  - PPP Passive Mode—Enabled or disabled
  - PPP Multilink—Enabled or disabled
  - PPP IPCP netmask option—Enabled or disabled
  - PPP max-negotiations IPCP—Maximum number of renegotiation attempts that the router accepts before terminating a PPP session
  - PPP AAA Profile—AAA profile associated with this PPP interface
  - PPP Multilink Fragmentation—Enabled or disabled
  - PPP Multilink Fragment Size—Multilink fragment size for this PPP interface
  - PPP Multilink Reassembly—Enabled or disabled
  - PPP Multilink Mrru—Multilink MRRU value for this PPP interface
  - PPP Initiate IP—Initiation of IPv4 over this PPP interface; enabled or disabled
  - PPP Initiate IPv6—Initiation of IPv6 over this PPP interface; enabled or disabled
  - PPPoE Max Sessions—Maximum number of PPPoE subinterfaces that can be on an interface
  - PPPoE Always-offer—Router offers to set up a session for the client, even if the router has insufficient resources to establish a session; enabled or disabled
  - PPPoE Remote-Circuit-Id—The router captures and processes a vendor-specific tag containing a remote circuit ID transmitted from a digital subscriber line access multiplexer (DSLAM); enabled or disabled
  - PPPoE Log PPPoeControlPacket—Enabled or disabled
  - PPPOE duplicate-protect—Enabled or disabled
  - PPPoE ACNAME—Access concentrator name
  - PPPoE URL—URL sent in PADM message to PPPoE clients
  - PPPoE MOTM—Message of the minute sent in the PADM message to PPPoE clients
  - PPPoE Service-Name Table—Name of the PPPoE service name table, if configured for the specified profile

  - ATM1483 Auto-configure—Whether autodetection of the specified upper-interface encapsulation type (bridged Ethernet, IP, PPP, or PPPoE) is enabled or disabled for a dynamic ATM 1483 subinterface
  - ATM1483 lockout (seconds)—Encapsulation type lockout setting for the specified upper-interface encapsulation type (bridged Ethernet, IP, PPP, or PPPoE) configured on a dynamic ATM 1483 subinterface
    - range—Minimum lockout time–maximum lockout time, in seconds
    - no lockout—Encapsulation type lockout is disabled
  - ATM1483 PVC circuit type—Encapsulation setting for the PVC configured on a dynamic ATM 1483 subinterface
    - aal5autoconfig—Enables autodetection of the 1483 encapsulation (LLC/SNAP or VC multiplexed)
    - aal5mux ip—VC-based multiplexed circuit for IP only
    - aal5snap—LLC encapsulated circuit; the LLC/SNAP header precedes the protocol datagram
  - ATM1483 PVC service category—Service type setting for the PVC configured on a dynamic ATM 1483 subinterface: UBR (the default), UBR PCR, NRT-VBR, RT-VBR, or CBR
  - ATM1483 PVC Peak rate—Peak cell rate (PCR), in Kbps, for the PVC configured on a dynamic ATM 1483 subinterfaces
  - ATM1483 PVC Avg rate—Average rate, in Kbps, for the PVC configured on a dynamic ATM 1483 subinterface; also referred to as sustained cell rate (SCR)
  - ATM1483 PVC Burst size—Length in cells of the burst for the PVC configured on a a dynamic ATM 1483 subinterface; also referred to as maximum burst size (MBS)
  - ATM1483 Description—Text description assigned to ATM 1483 subinterfaces that are created with this profile
  - ATM1483 Advisory Rx Speed—Configured receive speed, in Kbps, for the dynamic ATM 1483 subinterface. The E Series LAC sends this value to the LNS in the RX Connect-Speed AVP [38].
  - ATM1483 PVC OAM Administrative status—Status of OAM F5 loopback cell generation (for VC integrity) on a circuit created with this profile: enabled or disabled
  - ATM1483 PVC OAM Loopback frequency—Number of seconds between transmissions of OAM F5 end-to-end loopback cells on a circuit created with this profile
  - ATM1483 Ip Subscriber information—Subscriber login information for the specified dynamic interface type
  - ATM1483 Profile—Name of the profile assigned to the specified upper-interface encapsulation type (bridged Ethernet, IP, PPP, or PPPoE); these profiles are referenced in the base profile for a dynamic ATM 1483 subinterface as nested profile assignments
  - VLAN Auto-configure—Whether auto detection of the specified upper-interface encapsulation type (IP or PPPoE) is enabled or disabled for a dynamic VLAN subinterface
  - VLAN Advisory Rx Speed—Configured advisory receive speed, in Kbps, for the dynamic VLAN subinterface; the E Series LAC sends this value to the LNS in the RX Connect-Speed AVP [38]
  - VLAN Advisory Tx Speed—Configured advisory speed, in Kbps, for the dynamic VLAN subinterface.
  - VLAN Description—Text description assigned to VLAN subinterfaces that are created with this profile
  - VLAN Profile—Name of the profile assigned to the specified upper-interface encapsulation type (IP or PPPoE); these profiles are referenced in the base profile for a dynamic VLAN subinterface as nested profile assignments
  - VLAN Service Profile—Service profile name for a VLAN
  - VLAN Svlan Ethertype—Ethertype that the packet must use this to create the dynamic VLAN subinterface
  - Bridged Ethernet Mtu—MTU size configured for a dynamic bridged Ethernet interface
  - Bridged Ethernet Service Profile—Name of the IP service profile associated with the interface profile for this dynamic bridged Ethernet interface
  - IPv6 Unnumbered interface—Name of interface without a specific address
  - IPv6 Router—Router name or default
  - IPv6 Src-Addr Validation—Source-Address Validation; enabled or disabled
  - IPv6 Administrative MTU—MTU size
  - IPv6 ND Enabled—State of the Neighbor Discovery; enabled or disabled
  - IPv6 ND ManagedConfig—State of the Neighbor Discovery router advertisement managed flag; enabled or disabled
  - IPv6 ND OtherConfig—State of the Neighbor Discovery router advertisement other config flag; enabled or disabled
  - IPv6 ND SuppressRa—Status IPv6 router advertisement suppression; enabled or disabled
  - IPv6 ND RaInterval—Interval (in seconds) of the Neighbor Discovery router advertisement
  - IPv6 ND RaLifeTime—Lifetime (in seconds) of the Neighbor Discovery router advertisement
  - IPv6 ND ReachableTime—Amount of time (in milliseconds) that the neighbor is expected to remain reachable
  - IPv6 ND RaPrefix—Configured prefixes for Neighbor Discovery router advertisement
  - IPv6 ND ValidLifetime—Amount of time (in seconds) that the router advertises the IPv6 prefix as valid
  - IPv6 ND PreferredLifetime—Amount of time (in seconds) that the router advertises the specified IPv6 prefix as preferred
  - IPv6 ND PrefixOnLink—State of the on-link flag; enabled or disabled
  - IPv6 ND PrefixAutoConfig—State of the use the specified prefix for IPv6 autoconfiguration; enabled or disabled
- Example 1—Displays configuration information for a profile assigned to a dynamic interface

      host1#show profile name pppoeProfile
      Profile                    : pppoeProfile
      Unnumbered interface on    : loopback 1
      Router                     : default
      Directed Broadcast         : Disabled
      ICMP Redirects             : Disabled
      Access Route Addition      : Enabled
      Network Address Translation: Disabled
      Source-Address Validation  : Disabled
      Ignore DF Bit              : Disabled
      Filter Option Packets      : Disabled
      Administrative MTU         : 1500
      TCP MSS value              : 0
      Inactivity Timer           : Disabled
      Route Map Name             : Disabled
      Auto Detect                : Disabled
      Auto Configure             : Disabled

      IGMP                       : Enabled
        static-groups            :
        Input policy:  bobb statistics enabled
        Output policy: bobb statistics enabled

      PPP Keepalive               : 30
      PPP Magic Number            : enabled
      PPP Magic Number Mismatch   : ignore
      PPP Peer DNS Priority       : disabled
      PPP Peer WINS Priority      : disabled
      PPP Authentication          : pap/chap
      PPP Authentication Router   :
      PPP Negotiate MRU           : (use lower layer MRU)
      PPP Packet Log              : disabled
      PPP State Log               : disabled
      PPP Chap Challenge Length   : 16 - 32
      PPP Passive Mode            : disabled
      PPP Multilink               : disabled
      PPP IPCP Netmask Option     : disabled
      PPP max-negotiations IPCP   : 10
      PPP AAA Profile             :
      PPP Multilink Fragmentation : disabled
      PPP Multilink Fragment Size : (use MTU)
      PPP Multilink Reassembly    : disabled
      PPP Multilink Mrru          : (use MRU)
      PPP Initiate IP             : disabled
      PPP Initiate IPv6           : disabled
      PPPoE Max Sessions          : 2
      PPPoE Always-offer          : Disabled
      PPPoE Remote-Circuit-Id     : Enabled
      PPPoE Log PPPoeControlPacket: Disabled
      PPPoE duplicate-protect     : Enabled
      PPPoE ACNAME                : CYM9876
      PPPoE URL                   : http://www.urlofinterest.com
      PPPoE MOTM                  : goodmorning
      PPPoE Service-Name table    : myServiceTable1

- Example 2—Displays configuration information for a base profile assigned to a dynamic ATM 1483 subinterface

      host1#show profile name atm1483BaseProfile
      ATM1483 Auto-configure ip                 : disabled
      ATM1483 Auto-configure bridgedEthernet    : disabled
      ATM1483 Auto-configure ppp                : enabled
      ATM1483 lockout (seconds) ppp             : range : 1-300
      ATM1483 Auto-configure pppoe              : enabled
      ATM1483 lockout (seconds) pppoe           : range : 1-300
      ATM1483 PVC circuit type         :  aal5autoconfig
      ATM1483 PVC service category     :  Nrt-Vbr
      ATM1483 PVC Peak rate : 10000, Avg rate : 2000, Burst size : 500
      ATM1483 Description              :  VC_atm1483
      ATM1483 Advisory Rx Speed        :  2000000000

      ATM1483 PVC OAM Administrative status: enabled
      ATM1483 PVC OAM Loopback frequency:    30

      ATM1483 Ip Subscriber information:
        user             : elaine
        domain           : jpeterman.com
        password         : putty
      ATM1483 IP Profile               : none assigned
      ATM1483 Bridged Ethernet Profile : none assigned
      ATM1483 PPP Profile              : none assigned
      ATM1483 PPPoE Profile            : pppoeProfile

- Example 3—Displays configuration information for a base profile assigned to a dynamic VLAN subinterface

      host1#show profile name vlanProfile
      VLAN Auto-configure ip             : enabled
      VLAN Auto-configure pppoe          : enabled
      VLAN Svlan Ethertype               : auto-configure
      VLAN Advisory Rx Speed             : 100 Kbps
      VLAN Advisory Tx Speed             : 2500 Kbps
      VLAN Description                   : testing
      VLAN IP Profile                    : ipProfile
      VLAN PPPoE Profile                 : pppoeProfile
      VLAN Service Profile               : none assigned
      Bridged Ethernet Mtu               : 1971
      Bridged Ethernet Service Profile   : eastServiceProfile

- Example 4—Displays profile configuration information related to IPv6 Neighbor Discovery router advertisement

      host1#show profile name ipv6Profile
      IPv6 Unnumbered interface  : loopback 0
      IPv6 Router                : default
      IPv6 Src-Addr Validation   : Disabled
      IPv6 Administrative MTU    : 0
      IPv6 ND Enabled            : Enabled
      IPv6 ND ManagedConfig      : Disabled
      IPv6 ND OtherConfig        : Enabled
      IPv6 ND SuppressRa         : Disabled
      IPv6 ND RaInterval         : 50
      IPv6 ND RaLifeTime         : 1800
      IPv6 ND ReachableTime      : 0
      IPv6 ND RaPrefix           : 1234::/64
      IPv6 ND ValidLifetime      : 60
      IPv6 ND PreferredLifetime  : 60
      IPv6 ND PrefixOnLink       : Enabled
      IPv6 ND PrefixAutoConfig   : Enabled

- See show profile.

show vlan subinterface

- Use to display configuration and status information for a specified VLAN subinterface or for all VLAN subinterfaces configured on the router.
- Use the summary keyword to display only the counts of all VLAN subinterfaces and VLAN major interfaces configured on the router.
- Use the vlan or svlan keywords to display information about specific VLAN IDs or S-VLAN IDs.
- Field descriptions
  - Interface—Type and specifier of the VLAN subinterface
  - Status—Status of the VLAN subinterface: up, down, dormant, lowerLayerDown, absent
  - MTU—Maximum allowable size (in bytes) of the MTU for the VLAN subinterface
  - Svlan Id—S-VLAN ID value, if configured
  - Vlan Id—VLAN ID value for the VLAN subinterface
  - Ethertype—S-VLAN Ethertype value, if configured
  - Type—Type of VLAN subinterface
    - Static—VLAN or S-VLAN subinterface was configured statically
    - Dynamic—VLAN or S-VLAN subinterface was configured dynamically
  - Auto configure interface(s)—Types of dynamic upper interfaces configured with the auto-configure command: IP or PPPoE
  - Detected dynamic interface—Type of dynamic upper interface detected during autoconfiguration: IP, PPPoE, or (if no packet has been received) none
  - Interface types in lockout—Encapsulation types currently experiencing lockout: IP, PPPoE, or none
  - Lockout state (seconds)—Settings of encapsulation type lockout for the upper-layer encapsulation type indicated
    - Min—Minimum lockout time, in seconds
    - Max—Maximum lockout time, in seconds
    - Current—Current lockout time, in seconds; displays 0 (zero) if lockout is not occurring
    - Elapsed—Time elapsed into the lockout time, in seconds; displays 0 (zero) if lockout is not occurring
    - Next—Lockout time for the router to use for the next lockout event, in seconds
  - In—Analysis of inbound traffic on this interface
    - Bytes—Number of bytes received on the VLAN or S-VLAN subinterface
    - Packets—Sum of all unicast, broadcast, and multicast packets received on the VLAN or S-VLAN subinterface
    - Multicast—Number of multicast packets received on the VLAN or S-VLAN subinterface
    - Broadcast—Number of broadcast packets received on the VLAN or S-VLAN subinterface
    - Errors—Total number of errors in all received packets; some packets might contain more than one error
    - Discards—Total number of discarded incoming packets
  - Out—Analysis of outbound traffic on this interface
    - Bytes—Number of bytes sent on the VLAN or S-VLAN subinterface
    - Packets—Number of packets sent on the VLAN or S-VLAN subinterface
    - Multicast—Number of multicast packets received on the VLAN or S-VLAN subinterface
    - Broadcast—Number of broadcast packets received on the VLAN or S-VLAN subinterface
    - Errors—Total number of errors in all transmitted packets; some packets might contain more than one error
    - Discards—Total number of discarded outgoing packets
  - ARP Statistics—Analysis of ARP traffic on this interface; In fields are for traffic received on the interface and Out fields are for traffic sent on the interface
    - ARP requests—Number of ARP requests
    - ARP responses—Number of ARP responses
    - Errors—Total number of errors in all ARP packets
    - Discards—Total number of discarded ARP packets
  - Total VLAN interfaces—Total numbers of VLAN subinterfaces and VLAN major interfaces configured on the router; only this field appears when you specify the summary keyword
- Example 1—Displays full status and configuration information for all VLAN subinterfaces configured on the router

      host1#show vlan subinterface
              Interface        Status   MTU  Svlan Id Vlan Id  Ethertype  Type
      --------------------- ---------- ---- -------- -------- --------- -------
      ATM 3/0.1.2               Up       1522 ----     11       ----      Static
      ATM 3/0.1.3               Up       1522 ----     12       ----      Static
      ATM 3/1.1.1               Up       1522 ----     13       ----      Static
      ATM 3/1.1.2               Up       1522 ----     14       ----      Static
      ATM 3/2.1.1               Down     1526 4        255      0x9100    Static
      FastEthernet 4/5.1        Up       1522 ----     1        ----      Dynamic
      6 vlan subinterfaces found

- Example 2—Displays full status and configuration information for the specified VLAN subinterface

      host1#show vlan subinterface fastEthernet 4/5.1
              Interface       Status   MTU  Svlan Id Vlan Id  Ethertype  Type
      ---------------------- -------- ---- -------- -------- --------- -------
      FastEthernet 4/5.1        Up     522 ----       1       ----      Dynamic
      1 vlan subinterface found

- Example 3—Displays full status and configuration information for the specified S-VLAN ID

      host1#show vlan subinterface svlan id 100 53
              Interface       Status   MTU  Svlan Id Vlan Id Ethertype  Type
      ---------------------- -------- ---- -------- -------- --------- -------
      FastEthernet 0/0.1        Up     1526 100      53       0x9100    Static
      FastEthernet 4/6.1        Up     1526 100      53       0x9100    Dynamic
      2 vlan subinterfaces found

- Example 4—Displays full status and configuration information for the specified dynamic VLAN subinterface

      host1#show vlan subinterface fastEthernet 4/6.1000053
              Interface         Status  MTU  Svlan Id Vlan Id Ethertype Type
      ------------------------- ------ ---- -------- -------- --------- -------
      FastEthernet 4/6.1000053  Up      1526 100      53       0x9100   Dynamic
      Auto configure interface(s)   : IP  PPPoE
      Detected dynamic interface    : PPPoE
      Interface types in lockout    : none
      Lockout state (seconds)       : Min Max Current Elapsed Next
      ------------------------------- --- --- ------- ------- ----
      IP                                1 300       0       0    1
      PPPoE                             1 300       0       0    1
        In: Bytes 1040, Packets 15
         Multicast 0, Broadcast 1
         Errors 0, Discards 0
        Out: Bytes 984, Packets 15
         Multicast 0, Broadcast 1
         Errors 0, Discards 0
      ARP Statistics:
        In: ARP requests 0, ARP responses 0
         Errors 0, Discards 0
        Out: ARP requests 0, ARP responses 0
         Errors 0, Discards 0

- See show vlan subinterface.

[Contents] [Prev] [Next] [Index] [Report an Error]