[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls rsvp signalling hello graceful-restart

#### Syntax

{ ip | mpls } rsvp signalling hello graceful-restart [ mode help-neighbor ]

no { ip | mpls } rsvp signalling hello graceful-restart

#### Release Information

Command introduced in JUNOSe Release 8.0.0.

#### Description

Enables RSVP-TE graceful restart as a restarting node or helper node on the current virtual router. The no version disables graceful restart on the current VR.

#### Options

- ip—Specifies alternative keyword for compatibility with non–E Series implementations
- mode help-neighbor—Specifies the current VR acts only as a graceful restart helper node for neighbors that support RSVP-TE graceful restart

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]