[Contents] [Prev] [Next] [Index] [Report an Error]

# show frame-relay lip

#### Syntax

show frame-relay lip [ interface interfaceType interfaceSpecifier ] [ brief ] [ delta ]
[ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays Link Integrity Protocol state and statistics for a link in an MLFR bundle.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers :
  - serial
  - pos
- interfaceSpecifier—Particular interface in the format slot/port:link:
  - slot—Number of the chassis slot of the line module in the range 0–13 (ERX14xx models) and 0–6 (ERX7xx models)
  - port—Port number in the range 0–2
  - link—Number of a link in the range 1–8
- brief—Summarized format
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]