[Contents] [Prev] [Next] [Index] [Report an Error]

## Using SNMP Secure Packet Mirroring Traps

SNMP secure packet mirroring traps enable you to capture and report packet mirroring information to an external device; you can then view the secure information on the remote device. The secure packet mirroring traps feature is an extension of the router’s standard SNMP implementation, and is only available to SNMPv3 users who are authorized to use packet mirroring.

You can also log mirror traps to local volatile memory for debugging purposes by enabling the SNMP secure log feature. See Capturing SNMP Secure Audit Logs for details of secure audit logging. Normal console and syslog audit logs for packet mirroring traps and packet Mirror-MIB accesses are suppressed due to security concerns.

| Note: The contents of secure logs are not preserved across a reboot.

The mirror-enable command must be enabled to make packet mirroring-related commands, command options, and show command output visible.

| Note: You must use the CLI to configure the secure packet mirroring trap category to allow transmission of secure packet mirroring traps through the router—you cannot use SNMP to configure the secure packet mirroring trap category. However, after you have configured the secure packet mirroring trap category using the CLI, you can then use SNMP (juniPacketMirrorMIB.mi2) to enable and disable secure packet mirroring traps.

Table 57 indicates the events that trigger secure packet-mirroring traps and lists the information sent in the trap for each event.

Table 57: Packet-Mirroring SNMP Traps

Trap Information Sent | Event That Triggers the Trap
--- | ---
| A secure policy failed during CoA-based or RADIUS-initiated packet mirroring | A secure policy failed during CLI trigger or CLI-based packet mirroring | An interface with secure policies attached is deleted | An analyzer is unreachable
Analyzer address | – | – | – | ✓
Application name | ✓ | ✓ | – | –
Configuration source | ✓ | ✓ | ✓ | –
Date and time of event | – | ✓ | ✓ | ✓
Error cause | ✓ | ✓ | – | –
Error string | ✓ | ✓ | – | –
Mirror ID | ✓ | – | ✓ | –
Mirroring direction | – | – | ✓ | –
Secure policy name | – | ✓ | ✓ | –
Secure policy UID | – | ✓ | ✓ | –
Session ID | ✓ | – | ✓ | –
Trigger event | ✓ | ✓ | ✓ | –
Trigger type | ✓ | ✓ | ✓ | –
Username | ✓ | – | – | –
Virtual router (0 for L2TP) | ✓ | ✓ | ✓ | ✓

## Additional Packet-Mirroring Traps for CALEA Compliance

You can use the packet-mirroring traps shown in Table 58 to help support compliance with the Communications Assistance for Law Enforcement Act (CALEA), which defines electronic surveillance guidelines for telecommunications companies. For example, a third-party vendor of mediation devices might receive packet mirroring traps from the router and convert the traps to messages that comply with CALEA, such as Lawfully Authorized Electronic Surveillance (LAES) for IP Network Access, American Nation Standard For Telecommunications messages. Individual traps might map to multiple LAES messages to provide additional compliance-related information.

Table 58: Packet-Mirroring Traps for CALEA Compliance

Trap | Description
--- | ---
juniPacketMirrorSessionStart | A grant has been issued to a mirrored subscriber.
juniPacketMirrorSessionEnd | A mirrored session has been terminated; includes the termination reason.
juniPacketMirrorInterfaceSessionActivated | A secure policy has been attached to an existing interface or to an existing session.
juniPacketMirrorInterfaceSessionDeactivated | A secure policy has been detached from an interface, not including interface or session termination.
juniPacketMirrorSessionReject | A deny has been issued because the potential mirrored user was not allowed on the network for some reason. However, the user would have been mirrored if access to the network had been allowed.
juniPacketMirrorSessionFailed | The user session was terminated before the secure policy was attached. For example, no resources were available to create the interface. The termination reason is included.

## Packet Mirroring Trap Severity Levels

Table 59 lists the default severity levels for packet mirroring traps. See the JUNOSe System Basics Configuration Guide for descriptions of the severity levels.

Table 59: Packet Mirroring Trap Severity Levels

Trap | Default Severity Level
--- | ---
juniPacketMirrorAnalyzerUnreachable | Warning
juniPacketMirrorCliTriggerBasedMirroringFailure | Error
juniPacketMirrorInterfaceDeleted | Notice
juniPacketMirrorInterfaceSessionActivated | Info
juniPacketMirrorInterfaceSessionDeactivated | Info
juniPacketMirrorRadiusBasedMirroringFailure | Error
juniPacketMirrorSessionEnd | Info
juniPacketMirrorSessionFailed | Info
juniPacketMirrorSessionStart | Info
juniPacketMirrorSessionReject | Info

#### Related Topics

- See Configuring SNMP in JUNOSe System Basics Configuration Guide for information about JUNOSe software SNMP support.
- Configuring SNMP Secure Packet Mirroring Traps
- mirror trap-enable
- snmp-server clear secure-log
- snmp-server enable traps
- snmp-server host
- snmp-server secure-log
- show mirror trap
- show snmp secure-log

[Contents] [Prev] [Next] [Index] [Report an Error]