[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 ospf area

#### Syntax

[ no ] ip ospf [ processId ] area { areaId | areaIdInt }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates an OSPFv3 interface under the specified area ID or moves an OSPFv3 interface from its current area to a specified area. The no version removes the interface from the specified area.

#### Options

- processId—Integer in the range 1–65535
- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value 0–4294967295

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]