[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Configured Switch Profiles on Router

#### Purpose

Display information about the L2TP switch profiles configured on the router.

#### Action

To display only the names of the L2TP tunnel switch profiles configured on the router:

    host1#show l2tp switch-profile
    L2TP tunnel switch profile concord
    L2TP tunnel switch profile myProfile
    2 L2TP tunnel switch profiles found

To display information about the settings in a particular L2TP tunnel switch profile:

    host1#show l2tp switch-profile concord
    L2TP tunnel switch profile concord
      AVP bearer type action is relay
      AVP calling number action is relay
      AVP Cisco nas port info action is relay

#### Meaning

Table 90 lists the show l2tp switch-profile command output fields.

Table 90: show l2tp switch-profile Output Fields

Field Name | Field Description
--- | ---
L2TP tunnel switch profile | Name of the L2TP tunnel switch profile
AVP actionType action is | Indicates the tunnel switching behavior or action type (for example, relay) configured for the specified L2TP AVP type

#### Related Topics

- show l2tp switch-profile

[Contents] [Prev] [Next] [Index] [Report an Error]