[Contents] [Prev] [Next] [Report an Error]

# SRP-100 Module

> Module label | SRP-100
> IOA label | SRP IOA
> Number of IOA ports | Not applicable
> Software release | First supported: 7.0.1
> Description | 75 W Switch route processor (100 Gbps) Performs system management, route table calculations and maintenance, forwarding table computations, statistics processing, configuration storage, and other control plane functions Has 2 GB of memory Works with the SFM–100 module to create a switch fabric Uses a PCMCIA nonvolatile storage (NVS) card to store the system's software and configuration files Must be installed only with SRP-100 module and SFM–100 modules
> Capability | Not applicable
> Software features | Not applicable
> Model compatibility | E320 router
> Line module compatibility | ES2 4G LM ES2 10G UPLINK LM ES2 10G LM ES2 10G ADV LM (only in turbo slots)
> SRP module compatibility | Cannot use with SRP-120 module or SFM-120 module Cannot use with SRP-320 module or SFM-320 module
> Line module redundancy compatibility | Yes ( ES2-S1 REDUND IOA must be installed in either slot 0 or slot 11)
> Module redundancy support | 1:1 redundancy
> Port redundancy support | Not applicable
> Cables and connectors | Not applicable
> LEDs | Board-level LEDs: OK (green)—Self-test passed FAIL (red)—Failure detected ONLINE (green)—Online with no alarms or errors REDUN (green)—Module is the spare system controller, is up, and is ready to take the role of the online system controller. When LED is not lit, module is not acting as the spare system controller. PA (green)—Power source on source A PB (green)—Power source on source B FO (green)—Fan OK FF (red)—Fan failure LK (green)—Ethernet link up AC (green)—Blinks when there is Ethernet activity (traffic) on link Flash Card Port LEDs: 0 (green)—When lit, indicates slot is busy 1 (green)—When lit, indicates slot is busy
> Alarms, errors, and events | See Monitoring Modules in JUNOSe System Basics Configuration Guide, Chapter 6, Managing Modules.

[Contents] [Prev] [Next] [Report an Error]