[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

Symbols A B C D E F G H I M N O P R S T V

Symbols

> 144–bit CAM entries
>   example of IPv6 classifiers in a policy
>     supported by CAM classifiers 1
> 288–bit CAM entries
>   example of IPv6 classifiers in a policy
>     supported by CAM classifiers 1
> 576–bit CAM entries
>   example of IPv6 classifiers in a policy
>     supported by CAM classifiers 1

A

> access level
>   mirror-enable command 1
>   packet mirroring 1
> analyzer interfaces
>   interface types 1, 2
>   policies on 1
> atm commands
>   atm-cell-mode 1, 2
> attachment of IPv6 policies
>   to an interface
>     with CAM entries greater than 128 bits 1
> audit logging, SNMP secure 1, 2

B

> bandwidth management 1
> baseline commands
>   baseline radius dynamic-request 1

C

> CAM blocks
>   containing equal-sized CAM entries 1
>   support for variable-sized entries
>     1
>   utilization for CAM entries
>     in an IPv4 policy, example 1
>     in an IPv6 policy, example 1
> CAM device block size
>   division to hold CAM entries
>     example 1
> CAM entries
>   configured on line moduels
>     calculation of CAM bit size 1
>   division into blocks to store policies
>     example for GE-2 LMs 1
>   number per allocation
>     formula for scaling limits on GE-2 LMs 1
>     formula for scaling limits on GE-HDE LMs 1
>   obtaining length dynamically, three types
>     between 128 and 272 bits 1
>     between 272 and 336 bits 1
>     less than 128 bits 1
>   using the optimum size
>     for IPv6 policies 1
> CAM hardware classifiers
>   three types of CAM entries supported
>     on line modules of E Series Broadband Services Routers 1
>   variables-sized entries
>     for IPv6 policies 1
> CAM resources
>   and variable-sized CAM entries
>     factors used to determine availability 1
> classifier
>   CAM hardware 1, 2, 3
>   consumption 1
>   FPGA hardware 1, 2, 3
>   hardware 1, 2
>   line module support 1, 2, 3
>   policy consumption 1, 2
>   software 1, 2, 3
> classifier control list
>   criteria defined 1
>   matching IP flags 1
>   matching IP fragmentation offset 1
>   matching TCP flags 1
>   multiple elements in 1
> classifier groups
>   creating 1
> classifier-group commands
>   classifier-group 1
> color-aware configuration 1
> committed-action command 1
> committed-burst command 1
> conventions
>   notice icons 1
>   text and syntax 1
> customer support 1
>   contacting JTAC 1

D

> default classifier
>   allocation of CAM blocks
>     determined by the CAM entry size 1
>   consumption of CAM blocks
>     same as the size computed for the policy 1
> documentation set
>   comments on 1

E

> E320 routers
>   Ethernet interfaces 1
> exceeded-action command 1
> excess-burst command 1
> exp-mask command 1
> explicit packet coloring 1

F

> forward command 1, 2
> forward interface command 1
> forward next-hop command 1
> fragmentation offsets, filtering 1

G

> GE-2 line modules
>   formula for scaling numbers of
>     CAM entries 1
> GE-HDE line modules
>   formula for scaling limits
>     CAM entries 1

H

> hierarchical aggregation nodes 1
> hierarchical policing for interface groups 1

I

> interface mirroring
>   supported modules 1
> IP auxiliary input policy 1, 2
> ip commands
>   ip classifier-list 1
>   ipv6 classifier-list 1
> IP fragmentation
>   offset, matching in a policy 1
> IP options, filtering 1
> IP policies
>   scalability improvement for
>     using optimum CAM entry size 1
> IPv4 classifier
>   number of bits consumed
>     for CAM entries 1
> IPv6 classification
>   144–bit CAM entries
>     active classifiers in the example and size of each 1
>     example for a policy attachment 1
>   288–bit CAM entries
>     active classifiers in the example and size of each 1
>     example for a policy attachment 1
>   576–bit CAM entries
>     active classifiers in the example and size of each 1
>     example for a policy attachment 1
>     number of lookups to the CAM hardware 1
>   determination of fields in the classifier
>     using policy definition 1
>   minimum and maximum entry sizes
>     for IPv6 header CAM entries 1
>   support for traffic greater than 128 bits
>     1
>   variable-sized CAM entries
>     and available CAM resources 1
>     maximum policies supported with four classifier per policy 1
>     maximum policies supported with one classifier per policy 1
>     performance impact 1
> IPv6 classifier See IPv6 classification
> IPv6 policies
>   with four classifiers per policy
>     maximum supported with variable-sized CAM entries 1
>   with one classifier per policy
>     maximum supported with variable-sized CAM entries 1
> IPv6 policy definition
>   sum of classification fields in the
>     and variable-sized CAM entries 1

M

> manuals
>   comments on 1
> mark rule
>   with rate-limit rule 1
> mark-exp command 1, 2
> merged policy naming conventions 1
> merging policies 1
>   configuration example 1
>   error conditions 1
>   naming conventions 1
>   persistent configuration differences 1
>   policy attachment rules 1
>   policy attachment sequence 1
>   reference counting 1
>   resolving conflicts 1
>   restrictions 1
>   rules for attachment 1
> mirror-enable command
>   access level 1
>   and TACACS+ 1
> MTU (maximum transmission unit)
>   IP 1, 2
> multiple forwarding solutions 1

N

> notice icons 1

O

> one-rate rate-limit profile 1
> overlapping classification 1, 2

P

> packet coloring, explicit 1
> packet flow monitoring 1
> packet mirroring
>   access level 1
>   analyzer device 1
>   CLI-based 1, 2
>   configuration conflicts 1
>   configuring traps 1
>   interface-specific 1
>   ip analyzer interface 1
>   mediation device 1
>   multiple configurations 1
>   RADIUS-based 1
>   secure audit logging 1, 2
>   secure local logs 1
>   secure logging 1
>   secure SNMP traps 1
>   securing with TACACS+ 1
>   SNMP secure traps 1
>   system resources 1
>   terms 1
>   trigger 1
>   triggers for CLI-based 1
>   user-specific 1
> packet tagging 1
> parent group merge algorithm 1
> peak-burst command 1
> peak-rate command 1
> percent-based rates 1
> platform considerations
>   packet mirroring 1
> policies
>   analyzer interfaces 1
>   using RADIUS to create
>     overview 1
> policy attachment rules 1
> policy list
>   constructing a 1
>   creating or modifying 1
> policy lists
>   applying
>     overview 1
> policy management
>   applications
>     packet tagging 1
>   bandwidth management 1
>   baselining statistics 1
>   classifier groups, creating 1
>   classifier resources 1
>   committed burst calculation 1, 2
>   congestion management 1
>   creating a one-rate rate-limit profile 1
>   creating a two-rate rate-limit profile 1
>   explicit packet coloring 1
>   filtering fragmentation offsets 1
>   filtering IP options 1
>   matching IP flags in a CLACL 1
>   matching IP fragmentation offset in a CLACL 1
>   matching TCP flags in a CLACL 1
>   merging policies 1
>   modifying a one-rate rate-limit profile 1
>   modifying a two-rate rate-limit profile 1
>   monitoring packet flow 1, 2
>   one-rate rate-limit profile 1
>   overview 1
>   packet logging 1
>   packet mirroring 1
>   packet tagging 1, 2, 3
>   policy actions and rate-limit profiles 1
>   policy routing 1
>   policy rules, creating 1
>   QoS classification and marking 1
>   RADIUS support 1
>   rate limiting traffic flows 1
>   rate-limit profile actions 1
>   rate-limit profile attributes 1
>   rate-limit profile calculations 1
>   rate-limit profile defaults 1, 2
>   resources 1
>   security 1
> policy management configuration tasks 1
> policy parameter
>   considerations 1
>   quick configuration 1
>   reference-rate 1
> policy rule commands
>   forward 1
>   forward interface 1
>   forward next-hop 1
> policy rules
>   creating 1
>   precedence 1
>   supported commands 1

R

> rate limiting
>   aggregate traffic flows 1
>   for interfaces 1
>   hierarchical 1
>   individual traffic flows 1
> rate-limit hierarchies 1
>   classifier groups 1
>   color-aware configuration 1
>   rate-limit actions 1
>   rate-limit profiles 1
>   rate-limit rules 1
> rate-limit profiles
>   attributes 1
>   burst size 1
>   calculations 1
>   configuration procedure 1
>   creating 1, 2
>   default values 1, 2
>   modifying 1, 2
>   percent-based rates 1
>   policy actions 1
>   rates 1
> rate-limit rule
>   with mark rule 1
> rate-limit-profile one-rate command 1
> rate-limit-profile two-rate command 1
> rate-limiting SRP traffic flows 1
> resolving merge conflicts 1

S

> secure audit logging for packet mirroring 1, 2
> secure policy-list command 1
> Service Manager
>   merging policies 1
> show commands
>   show color-mark-profile 1
>   show control-plane policer 1
>   show frame-relay subinterface 1
>   show gre tunnel 1
>   show interfaces 1
>   show ipv6 interface 1
>   show parent-group 1, 2, 3, 4, 5
>   show policy-parameter 1
>   show rate-limit-profile 1
>   show secure classifier-list 1
>   show vlan subinterfaces 1, 2
> show ip commands
>   show ip interface 1, 2
>   show ip mirror interface 1
> show mirror commands
>   show mirror log 1, 2
>   show mirror rules 1
>   show mirror subscribers 1
> show radius commands
>   show radius servers 1
>   show radius statistics 1
> show secure policy-list command 1
> show snmp commands
>   show snmp secure-log 1
>   show snmp trap 1
> single-rate rate limit profile 1
> SNMP (Simple Network Management Protocol)
>   secure audit logs 1, 2
> SNMP traps 1
>   secure logs 1
> support, technical See technical support

T

> TCP-friendly one-rate rate-limit profile 1
> technical support
>   contacting JTAC 1
> text and syntax conventions 1
> traffic-class command 1
> traps, SNMP
>   status information 1
> two-rate rate-limit profile 1

V

> variable length IPv6 classifiers
>   examples of
>     supported CAM entries 1
> variable-sized CAM entries
>   144–bit size
>     active classifiers in the example policy 1
>     creation and attachment of an IPv6 policy, example 1
>     size of each classifier in the IPv6 policy example 1
>   288–bit size
>     active classifiers in the example policy 1
>     creation and attachment of an IPv6 policy, example 1
>     size of each classifier in the IPv6 policy example 1
>   576–bit size
>     active classifiers in the example policy 1
>     creation and attachment of an IPv6 policy, example 1
>     size of each classifier in the IPv6 policy example 1
>   factors to determine
>     available CAM resources 1
>   for IPv6 classification
>     supported bit sizes 1
>   maximum IPv6 policies supported
>     with four classifiers per policy 1
>     with one classifier per policy 1
>   performance impact
>     caused by CAM addressing 1

[Contents] [Prev] [Next] [Index] [Report an Error]