> - radius override nas-info

> # radius override nas-info

> #### Syntax

> [ no ] radius override nas-info

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the RADIUS client for a virtual router context to override the standard use of the NAS-IP-Address [4] and NAS-Identifier [32] attributes when the client performs AAA broadcast accounting. Normally, AAA accounting packets include the NAS-IP-Address and NAS-Identifier attributes of the virtual router that generates the accounting information. However, this command specifies that the broadcast accounting packets instead include the authenticating virtual router’s NAS-IP-Address and NAS-Identifier attributes. The no version restores the standard use of the two attributes in AAA accounting information.

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.