[Contents] [Prev] [Next] [Index] [Report an Error]

## Configuring IGMP

IP hosts use Internet Group Management Protocol (IGMP) in IPv4 to report their multicast group memberships to neighboring routers. Similarly, multicast routers, such as an E Series router, use IGMP to discover which of their hosts belong to multicast groups.

This chapter describes how to configure IGMP for IP multicast on an E Series router; it contains the following sections:

- IGMP Overview
- Platform Considerations
- References
- Before You Begin
- Configuring Static and Dynamic IGMP Interfaces
- Enabling IGMP on an Interface
- Configuring IGMP Settings for an Interface
- Specifying Multicast Groups
- Assigning a Multicast Group to an Interface
- Configuring Group Outgoing Interface Mapping
- Configuring Access Node Control Protocol for IGMP
- Configuring SSM Mapping
- Limiting the Number of Accepted IGMP Groups
- Including and Excluding Traffic
- Configuring Explicit Host Tracking
- Accepting IGMP Reports from Remote Subnetworks
- Disabling and Removing IGMP
- Monitoring IGMP
- IGMP Proxy Overview
- Configuring IGMP Proxy
- Establishing the IGMP Proxy Baseline
- Monitoring IGMP Proxy

[Contents] [Prev] [Next] [Index] [Report an Error]