> - arp spoof-check

> # arp spoof-check

> #### Syntax

> [ no ] arp spoof-check

> #### Release Information

> Command introduced in JUNOSe Release 9.3.0.

> #### Description

> Configures the router to check for spoofed ARP packets received on an IP interface. By default, the router checks all ARP packets received on a major IP interface or a subinterface to identify and discard spoofed ARP packets. The no version disables checking for spoofed ARP packets received on the interface.

> #### Mode

> Interface Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.