[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

Symbols A B C D E F G H I J K L M N O P R S T U V W X

Symbols

> 10-Gigabit Ethernet interfaces
>   modules 1
>   specifying an interface 1
> 4xDS3 ATM I/O modules 1

A

> Address Resolution Protocol. See ARP
> all option (show controllers) 1, 2
> aps commands 1
>   aps events 1
>   aps force 1
>   aps group 1, 2
>   aps lockout 1
>   aps manual 1
>   aps protect 1
>   aps revert 1
>   aps unidirectional 1
>   aps working 1
>   See also show aps commands
> APS/MSP (Automatic Protect Switching/Multiplex Section Protection)
>   automatic switchover 1
>   channel numbers 1, 2
>   communication methods 1
>   configuration example 1
>   configuring 1, 2
>   events 1
>   K1 byte 1
>   K2 byte 1
>   manual switchover 1, 2
>   monitoring 1, 2
>   overview 1
>   protect interface 1, 2, 3, 4
>   reversion after switchover 1
>   switching mechanisms 1
>   working interface 1, 2, 3, 4
> ARP (Address Resolution Protocol) 1
> Automatic Protect Switching. See APS/MSP

B

> baseline commands
>   baseline interface 1
>   baseline interface serial
>     channelized T3 interfaces 1
>     cOCx/STMx interfaces 1
>     E3/T3 interfaces 1
>   baseline line interface sonet 1, 2
>   baseline path interface sonet 1, 2
>   baseline section interface sonet 1, 2
> BERT (bit error rate test) patterns
>   channelized T3 interfaces 1, 2, 3
>   cOCx/STMx interfaces 1, 2, 3
>   E3/T3 interfaces 1, 2
> bert command
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
> bit error rate test patterns. See BERT patterns

C

> cable length
>   specifying 1, 2
> cablelength commands
>   cablelength 1, 2
> cell scrambling
>   E3 1
>   T3 1
> channel numbers, APS/MSP interfaces 1, 2
> channel-group commands. See path ds1 | e1 commands
> channelized OCx/STMx interfaces. See cOCx/STMx interfaces
> channelized T3 interfaces
>   bert command 1
>   configuring 1, 2
>   configuring HDLC channel 1
>   equipment loopback command 1
>   loopback command 1
>   monitoring parameters 1
>   numbering scheme 1, 2
>   references 1
>   testing 1, 2
> clock commands
>   clock source
>     channelized T3 interfaces 1, 2
>     cOCx/STMx interfaces 1, 2
>     E3/T3 interfaces 1, 2
>     OCx/STMx interfaces 1
> clock source, selecting
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1
>   E1 interfaces on cOCx/STMx 1
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1, 2
>   T1 interfaces on cOCx/STMx 1
>   T3 interfaces on cOCx/STMx 1
> COCX-F3 line modules 1
> cOCx/STMx interfaces
>   configuring HDLC channel 1
>   configuring T1/E1 1
>   loopback 1, 2, 3, 4
>   monitoring 1
>   numbering scheme 1
>   references 1
>   testing 1, 2
> configuring. See specific feature, product, or protocol
> connectivity in SONET/SDH paths 1, 2
> control traffic for high-density Ethernet 1
> controller commands
>   controller e3 1, 2
>   controller sonet 1, 2
>   controller t3 1, 2, 3, 4
> conventions
>   notice icons 1
>   text and syntax 1
> counters
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
> CRC (cyclic redundancy check)
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> crc command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> CT3/T3 12 I/O modules 1
> CT3/T3 12 line modules 1
> CT3/T3-F0 line modules 1
> customer support 1
>   contacting JTAC 1
> cyclic redundancy check. See CRC

D

> data stream inversion, enabling
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> debounce command 1
> debounce-interval command 1
> dedicated tunnel-server ports
>   configuring 1
>   supported applications 1
>   supported modules 1
> description command
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
>   unchannelized SONET interfaces 1, 2
> description, interface
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1, 2, 3, 4
>   E3/T3 interfaces 1
>   serial interfaces 1, 2, 3
>   unchannelized SONET interfaces 1, 2
> Distance Vector Multicast Routing Protocol. See DVMRP tunnels
> documentation set
>   comments on 1
> DS0 timeslots
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1, 2, 3
> DS1. See T1 entries
> ds3-scramble command 1
> DS3. See T3 entries
> dsu commands
>   dsu bandwidth 1
>   dsu mode 1
> duplex command 1
> DVMRP tunnels 1
> dynamic tunnel-server ports
>   applications supported 1
>   overview 1
>   unprovisioning 1
> dynamic tunnel-service interfaces
>   monitoring 1
>   overview 1

E

> E1 channels
>   cOCx/STMx interfaces 1
> E1 interfaces. See cOCx/STMx interfaces
> E120 and E320 Broadband Services Routers
>   Ethernet interfaces 1
>   tunnel-service interfaces 1
> E120 Broadband Services Routers 1, 2
> E3 interfaces
>   configuring controllers 1
>   configuring HDLC channel 1
>   loopback command 1
>   monitoring interfaces 1
>   references 1
> e3-scramble command 1
> E320 Broadband Services Routers 1, 2, 3
>   100 Gbps fabric 1, 2
>   120 Gbps fabric 1
>   320 Gbps fabric 1, 2
> equipment loopback command
>   channelized T3 interfaces 1
>   T3 interfaces 1
> ES2 10G ADV line module (LM) 1
> ES2 10G line module (LM) 1, 2, 3, 4
> ES2 10G Uplink line module (LM) 1
> ES2 4G line module (LM) 1, 2, 3, 4
> ethernet description command 1
> Ethernet interfaces
>   commands 1
>     ethernet description 1
>     interface fastEthernet 1
>     interface gigabitEthernet 1
>     interface tenGigabitEthernet 1
>     See also show commands
>   configuring 1
>   debounce, enabling 1
>   debounce-interval, modifying 1
>   disabling interfaces 1
>   duplex type 1
>   high-density 1
>   IEEE 802.3ae 1, 2
>   line speed 1
>   MAC address validation 1
>   monitoring 1
>   numbering scheme 1, 2
> events
>   APS/MSP 1

F

> facilities data link. See FDL
> Fast Ethernet interfaces
>   modules 1
>   specifying an interface 1
> FDL (facilities data link)
>   cOCx/STMx interfaces 1
>     monitoring statistics 1
>     T1 channel over DS3, configuring 1
>     T1 over VT, configuring 1
>   T1 channels on channelized T3 interfaces 1
>     configuring 1
>     monitoring statistics 1
> filtering
>   show displays 1, 2, 3
> fractional T1/E1 1
> fractional T3 1
> framing command
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
> framing format
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1, 2
>   E3/T3 line 1

G

> Generic Routing Encapsulation. See GRE tunnels
> Gigabit Ethernet interfaces
>   modules 1
>   redundant port 1, 2
>   specifying an interface 1
> GRE (Generic Routing Encapsulation) tunnels 1

H

> HDLC channel, configuring
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> high-density Ethernet
>   overview 1
>   packet classifier 1
>   supported modules 1, 2, 3, 4

I

> idle character
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1, 2
>   E3/T3 interfaces 1
> idle-character command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1, 2
>   E3/T3 interfaces 1
> IEEE 802.1w 1
> IEEE 802.3ae 1, 2
> IEEE 802.3u 1
> IEEE 802.3z 1
> intelligent dropping of packets 1
> interface commands
>   interface fastEthernet 1
>   interface gigabitEthernet 1
>   interface serial
>     channelized T3 interfaces 1
>     cOCx/STMx interfaces 1
>     E3/T3 interfaces 1
>   interface tenGigabitEthernet 1
> interface description
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1, 2, 3, 4
>   E3/T3 interfaces 1
>   serial interfaces 1, 2, 3
>   unchannelized SONET interfaces 1, 2
> interface stack
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
>   ES2-21 OC48/STM16 POS 1
>   OCx/STMx POS interfaces 1
>   OCx/STMx/DS3-ATM interfaces 1
> interfaces, monitoring
>   channelized T3 1
>   cOCx/STMx 1
>   E3/T3 1
>   Ethernet 1
>   OCx/STMx 1
> internal clocking 1
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1, 2
>   E1 interfaces 1, 2
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1
>   T1 interfaces 1, 2
> invert data command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> ip commands
>   ip mac-validate 1
> IP tunnels
>   secure 1, 2
> ISMs (IPSec Service modules)
>   monitoring 1
>   redundancy and interface distribution 1

J

> Juniper Networks E320 Broadband Services Routers
>   SONET/SDH interfaces 1

K

> K1 byte, APS/MSP 1
> K2 byte, APS/MSP 1

L

> L2TP (Layer 2 Tunneling Protocol) 1
> L2TP network server. See LNS
> Layer 2 Tunneling Protocol. See L2TP
> line clocking 1, 2
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1, 2
>   E1interfaces 1, 2
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1
>   T1 interfaces 1, 2
> line modules
>   changing 1, 2
> line speed 1
> link commands
>   link failover force 1
>   link failover timeout 1
>   link selection 1
> LNS (L2TP network server)
>   termination 1
> load-interval command
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
>   Ethernet interfaces 1
> local loopback
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1
> loopback
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1, 2
>   E3/T3 interfaces 1
>   T3 interfaces, remote 1
> loopback command
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1

M

> MAC (media access control) addresses
>   validation 1
> MAC pause frames 1
> maintenance data link. See MDL
> manual switchover, APS/MSP 1
> manuals
>   comments on 1
> max-interfaces command 1
> maximum receive unit. See MRU
> maximum transmission unit. See MTU
> MDL (maintenance data link)
>   channelized T3 interfaces 1
>     configuring 1
>     monitoring statistics 1
>   T3 interfaces 1
>     configuring 1
>     monitoring statistics 1
>   T3 on cOCx/STMx interfaces 1
>     configuring 1
>     monitoring statistics 1
> mdl commands
>   mdl carrier 1, 2
>   mdl string 1, 2
>   mdl transmit 1, 2
> monitoring. See specific feature, product, or protocol
> MPLS (Multiprotocol Label Switching)
>   fast reroute 1, 2
> MRU (maximum receive unit)
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> mru command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> MSP 1
> MSP (Multiplex Section Protection) 1, 2
> MTU (maximum transmission unit)
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
>   Ethernet interfaces 1
> mtu command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
>   Ethernet interfaces 1, 2
> Multiplex Section Protection. See APS/MSP
> Multiprotocol Label Switching. See MPLS

N

> network loopback
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1
> notice icons 1
> numbering scheme
>   ASP/MSP 1, 2
>   slot/adapter/port 1, 2, 3
>   slot/port 1, 2, 3, 4, 5

O

> OC12 I/O modules 1, 2
> OC3-2 GE APS I/O module 1, 2
> OC3-4 I/O modules 1, 2, 3
> OC3/STM1 GE/FE line module 1, 2
> OCx/STMx interfaces
>   configuring 1, 2
>   disabling 1
>   line modules 1
>   monitoring statistics 1
>   numbering scheme 1
>   path ds3 loopback remote command 1
>   testing 1
> OCx/STMx POS line modules 1, 2
> OCx/STMx/DS3-ATM line modules 1, 2

P

> packet classifier 1
> packets
>   intelligently dropping 1
> path commands
>   path 1
>   path description 1, 2
>   path e1 unframed 1
>   path overhead c2 1, 2
>   path overhead j1 1, 2
>   path snmp trap link-status 1, 2
>   path trigger alarm 1, 2
>   path trigger delay 1, 2
> path ds1 fdl commands
>   path ds1 fdl 1
>   path ds1 fdl carrier 1
>   path ds1 fdl transmit 1
> path ds1 remote-loopback command 1
> path ds1|e1 commands
>   path ds1|e1 1
>   path ds1|e1 bert 1
>   path ds1|e1 channel-group description 1
>   path ds1|e1 channel-group shutdown 1
>   path ds1|e1 channel-group snmp trap link-status 1
>   path ds1|e1 channel-group timeslots 1
>   path ds1|e1 clock source 1
>   path ds1|e1 description 1
>   path ds1|e1 framing 1
>   path ds1|e1 loopback 1
>   path ds1|e1 loopback remote 1
>   path ds1|e1 shutdown 1
>   path ds1|e1 snmp trap link-status 1
> path ds3 commands
>   path ds3 1
>   path ds3 bert 1
>   path ds3 clock source 1
>   path ds3 description 1
>   path ds3 framing 1
>   path ds3 loopback 1
>   path ds3 loopback remote 1
>   path ds3 shutdown 1
>   path ds3 snmp trap link-status 1, 2
> path ds3 mdl commands
>   path ds3 mdl carrier 1
>   path ds3 mdl string 1
>   path ds3 mdl transmit 1
> path ds3 t1 commands
>   path ds3 t1 1
>   path ds3 t1 bert 1
>   path ds3 t1 clock source 1
>   path ds3 t1 description 1
>   path ds3 t1 framing 1
>   path ds3 t1 loopback 1
>   path ds3 t1 loopback remote 1
>   path ds3 t1 remote-loopback 1
>   path ds3 t1 shutdown 1
>   path ds3 t1 snmp trap link-status 1
>   path ds3 t1 timeslots 1
> path ds3 t1 fdl commands
>   path ds3 t1 fdl 1
>   path ds3 t1 fdl carrier 1
>   path ds3 t1 fdl transmit 1
> pause frames 1
> payload loopback
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
> platform considerations
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   Ethernet interfaces 1
>   tunnel-service interfaces 1
>   unchannelized SONET/SDH interfaces 1
>   unchannelized T3/E3 interfaces 1
> ports, tunnel-server
>   shared 1
> protect interface, APS/MSP 1, 2

R

> redundant port, Gigabit Ethernet 1, 2
> remote loopback
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   T3 interfaces 1, 2
> reversion
>   after switchover
>     APS/MSP 1
> RSTP (Rapid Spanning Tree Protocol) 1

S

> scramble command 1
> sdh command 1, 2
> section layer, SONET/SDH 1
> secure IP tunnels 1, 2
> serial description command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   E3/T3 interfaces 1
> serial interfaces
>   configuring
>     channelized T3 interfaces 1
>     cOCx/STMx interfaces 1
>     E3/T3 interfaces 1
>   monitoring
>     channelized T3 interfaces 1
>     cOCx/STMx 1
> SFPs (small form-factor pluggable transceivers) 1, 2
> shared tunnel-server ports
>   configuring 1
>   overview 1
>   supported applications 1
>   supported modules 1
> show aps commands
>   show aps 1
>   show aps group 1
> show controllers commands
>   show controllers e3 1
>   show controllers sonet 1
>   show controllers sonet configuration 1
>   show controllers sonet ds1|e1 1
>   show controllers sonet ds3 1
>   show controllers sonet line | path | section 1
>   show controllers sonet line | path | section | tributary 1
>   show controllers t3 1, 2
>   show controllers t3 ft1 1
>   show controllers t3 remote 1, 2, 3
>   show controllers t3 serial 1
> show displays, filtering 1, 2, 3
> show interfaces commands
>   show interfaces fastEthernet 1
>   show interfaces gigabitEthernet 1
>   show interfaces serial
>     channelized T3 interfaces 1
>     cOCx/STMx interfaces 1
>   show interfaces tenGigabitEthernet 1
> show tunnel-server command 1
> shutdown command
>   channelized T3 interfaces 1
>   E3/T3 interfaces 1
>   Ethernet interfaces 1
>   OCx/STMx interfaces 1
> shutting down
>   DS3 1
>   E3/T3 interfaces 1
>   SONET/SDH interface 1
>   T1 channel 1, 2
>   T1 subchannel 1, 2
>   T1/E1 channel 1
>   T1/E1 channel group 1
>   T3 controller 1
> SMs (Service modules)
>   monitoring 1
>   redundancy and interface distribution 1
> SNMP (Simple Network Management Protocol) link status processing
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1, 2, 3, 4, 5, 6
>   OCx/STMx interfaces 1, 2
> snmp trap link-status command
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   OCx/STMx interfaces 1
> SONET APS 1+1 redundancy. See APS/MSP
> SONET/SDH (synchronous optical network/Synchronous Digital Hierarchy)
>   alarms, configuring 1
>   line modules supported 1
>   MPLS fast reroute 1, 2
> source, clock
>   channelized T3 interfaces 1, 2
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1, 2
> speed command 1, 2
> static tunnel-service interfaces
>   monitoring 1
>   overview 1
> subchannels
>   configuring 1
>   monitoring 1
>   shutting down t1 1
> support, technical See technical support
> switching mechanisms, APS/MSP 1, 2
> switchover
>   APS/MSP 1
> Synchronous Digital Hierarchy. See SONET/SDH
> synchronous optical network. See SONET/SDH

T

> T1 channels
>   channelized T3 interfaces 1
>   cOCx/STMx interfaces 1
>   configuring 1
> t1 commands
>   t1 bert 1
>   t1 clock source 1
>   t1 description 1
>   t1 framing 1
>   t1 loopback 1
>   t1 remote-loopback 1
>   t1 shutdown 1
>   t1 snmp trap link-status 1
>   t1 timeslots 1
>   t1 yellow detect 1
>   t1 yellow generate 1
> t1 fdl commands
>   t1 fdl 1
>   t1 fdl carrier 1
>   t1 fdl string 1
>   t1 fdl transmit 1
> T3 channels 1
> T3 controllers
>   configuring 1
>   monitoring 1
> T3 interfaces
>   configuring controllers 1
>   configuring HDLC channel 1
>   configuring MDL 1
>   equipment loopback command 1
>   loopback command 1
>   monitoring 1
>   numbering scheme 1
>   testing 1
> T3, fractional 1
> technical support
>   contacting JTAC 1
> testing interfaces
>   channelized T3 1, 2
>   cOCx/STMx 1, 2
>   OCx/STMx 1, 2
> text and syntax conventions 1
> threshold command 1, 2
> time intervals 1, 2
> transmit clock source, configuring
>   channelized T3 interfaces 1, 2
>   cOCx/STMx interfaces 1, 2
>   E3/T3 interfaces 1
>   OCx/STMx interfaces 1, 2
> transmit powers and cable length 1, 2
> trigger delay command 1
> tunnel-server ports
>   dedicated 1
>   shared 1
> tunnel-service interfaces
>   configuring 1, 2
>   considerations 1
>   E120 and E320 Broadband Services Routers 1
>   monitoring 1
>   overview 1
>   redundancy and interface distribution 1, 2
> tunnels
>   configuring tunnel-service interfaces 1
>   dynamic tunnel-server ports 1
>   monitoring 1
>   secure IP 1, 2

U

> unframed E1 1

V

> VT (virtual tributary) 1

W

> working interface, APS/MSP 1, 2

X

> XFPs (10-gigabit small form-factor pluggable transceivers) 1, 2, 3

[Contents] [Prev] [Next] [Index] [Report an Error]