[Contents] [Prev] [Next] [Index] [Report an Error]

# ip nfs

#### Syntax

ip nfs { source-address ipAddress
| source-interface interfaceType interfaceSpecifier }

no ip nfs { source-address | source-interface }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the E Series interface that the current virtual router uses to exchange NFS communications with an NFS server. The no version prevents this interface from sending or receiving NFS communications for the current virtual router.

#### Options

- ipAddress—IP address of an E Series interface that sends and receives NFS communications
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]